<!DOCTYPE ServiceMan PUBLIC "-//CEMA//DTD CEMA Service Manual Modular 980431//EN" [
<!ENTITY % nparcon  "(Title? , (SafetyPara | Para | Para1 | Para2 | Para3 | Para4 | Para5 | Example)*)" --<Title>nparcon-- >

<!ELEMENT (Para1 | Para2 | Para3 | Para4 | Para5)  - - (((#PCDATA) | CrossRef | indxflag | change | emphasis | symbol | graphic | Link | subscrpt | supscrpt) | (seqlist | randlist | deflist))+ --<Title>Para-- >

<!ENTITY % mod SYSTEM "module.ent">
%mod;
<!ENTITY % ent SYSTEM "entity.ent">
%ent;
<!ENTITY hotspot SYSTEM "hotspot.ent">
]>
<ServiceMan>
<ManageInfo>
<Ident>
<Category>
</Category>
<Model>SA-HT623EE/SA-HT623GCS/SA-HT623GCU/SA-HT888GCA</Model>
<System>ORDER NO.CHM0408010C3 </System>
<SubSystem>DVD Home Theater Sound System </SubSystem>
<DataType></DataType>
</Ident>
<Status>
<ModuleTitle>s1207010000</ModuleTitle>
<IssueNo issue=1>
<IssueDate day=10 month=Aug year=2004>
<qa>
<Unverif>
</qa>
<ModelName>
<Name>SA-HT623EE/SA-HT623GCS/SA-HT623GCU/SA-HT888GCA</Name>
<SubModelName></SubModelName>
</ModelName>
<PubType pubtype=ServMan>
<Manufacturer></Manufacturer>
<Originator></Originator>
<Author></Author>
<Authorization>
<Language lang=Eng>
</Status>
</ManageInfo>
<content>
<ServMan>
<References><NoRefs></References>

<Body>
<Descriptive>
<Title>12.7.1 Precautions in optical pickup replacement</Title>
<Para>
<link linkend="ex-top">TOP</link>
<nameloc id="ex-top">
<nmlist nametype="entity">
ht623ee
</nmlist>
</nameloc>
<link linkend="ex-previous">PREVIOUS</link>
<nameloc id="ex-previous">
<nmlist nametype="entity">
s1207000000
</nmlist>
</nameloc>
<link linkend="ex-next">NEXT</link>
<nameloc id="ex-next">
<nmlist nametype="entity">
s1207020000
</nmlist>
</nameloc>
</Para>
<Para><emphasis>The optical pickup can be damaged by static electricity from you body. Be sure to take static electricity countermeasures when working around the optical pickup. (Refer to the related page in this Manual about the countermeasures.)</emphasis></Para>
<Para><seqlist><item><Para>Do not touch laser diode, actuator and their peripheries.</Para>
</item>
<item><Para> Do not use tester to check laser diode. (Laser diode can be damaged easily.)</Para>
</item>
<item><Para>The use of soldering iron with anti-static feature is recommended when providing short-circuit to laser diode or when removing it.</Para>
</item>
<item><Para>Solder the land on flexible cable of optical pickup unit.</Para>
<Para><emphasis>Caution</emphasis></Para>
<Para><randlist prefix=unorder><item><Para> When using the soldering iron without anti-static feature, short-circuit the flexible cable terminal with a clip before short-circuiting the land.</Para>
</item>
<item><Para>After intended repair is finished, remove the solder for short-circuit of laser diode in a correct way following the procedures described in this Manual.</Para>
</item>
</randlist>
</Para>
<Figure><graphic boardno="graphic57" reprowid="127.593mm" reprodep="63.500mm" location="internal"></Figure>
</item>
</seqlist>
</Para>

<!-- Footer -->

<Para>
<link linkend="bex-top">TOP</link>
<nameloc id="bex-top">
<nmlist nametype="entity">
ht623ee
</nmlist>
</nameloc>
<link linkend="bex-previous">PREVIOUS</link>
<nameloc id="bex-previous">
<nmlist nametype="entity">
s1207000000
</nmlist>
</nameloc>
<link linkend="bex-next">NEXT</link>
<nameloc id="bex-next">
<nmlist nametype="entity">
s1207020000
</nmlist>
</nameloc>
</Para>
</Descriptive>

&hotspot;
</Body>
</ServMan>
</content>
</ServiceMan>
