<!DOCTYPE ServiceMan PUBLIC "-//CEMA//DTD CEMA Service Manual Modular 980431//EN" [
<!ENTITY % nparcon  "(Title? , (SafetyPara | Para | Para1 | Para2 | Para3 | Para4 | Para5 | Example)*)" --<Title>nparcon-- >

<!ELEMENT (Para1 | Para2 | Para3 | Para4 | Para5)  - - (((#PCDATA) | CrossRef | indxflag | change | emphasis | symbol | graphic | Link | subscrpt | supscrpt) | (seqlist | randlist | deflist))+ --<Title>Para-- >

<!ENTITY % mod SYSTEM "module.ent">
%mod;
<!ENTITY % ent SYSTEM "entity.ent">
%ent;
<!ENTITY hotspot SYSTEM "hotspot.ent">
]>
<ServiceMan>
<ManageInfo>
<Ident>
<Category>
</Category>
<Model>SA-HT623EE/SA-HT623GCS/SA-HT623GCU/SA-HT888GCA</Model>
<System>ORDER NO.CHM0408010C3 </System>
<SubSystem>DVD Home Theater Sound System </SubSystem>
<DataType></DataType>
</Ident>
<Status>
<ModuleTitle>s1001000000</ModuleTitle>
<IssueNo issue=1>
<IssueDate day=10 month=Aug year=2004>
<qa>
<Unverif>
</qa>
<ModelName>
<Name>SA-HT623EE/SA-HT623GCS/SA-HT623GCU/SA-HT888GCA</Name>
<SubModelName></SubModelName>
</ModelName>
<PubType pubtype=ServMan>
<Manufacturer></Manufacturer>
<Originator></Originator>
<Author></Author>
<Authorization>
<Language lang=Eng>
</Status>
</ManageInfo>
<content>
<ServMan>
<References><NoRefs></References>

<Body>
<Descriptive>
<Title>10.1 Cautions to Be Taken in Handling the Optical Pickup Unit</Title>
<Para>
<link linkend="ex-top">TOP</link>
<nameloc id="ex-top">
<nmlist nametype="entity">
ht623ee
</nmlist>
</nameloc>
<link linkend="ex-previous">PREVIOUS</link>
<nameloc id="ex-previous">
<nmlist nametype="entity">
s1000000000x
</nmlist>
</nameloc>
<link linkend="ex-next">NEXT</link>
<nameloc id="ex-next">
<nmlist nametype="entity">
s1002000000
</nmlist>
</nameloc>
</Para>
<Para>The laser diode in the optical pickup unit may be damaged due to electrostatic discharge generating from clothes or human body. Use due caution to electrostatic discharge damage when servicing the laser diode.</Para>
<Para><seqlist><item><Para>Do not give a considerable shock to the optical pickup unit as it has an extremely high-precise structure.</Para>
</item>
<item><Para>To prevent the laser diode from the electrostatic discharge damage, the flexible cable of the optical pickup unit removed from the PCB should be short-circuited with a short pin or a clip.</Para>
</item>
<item><Para>The flexible cable may be cut off if an excessive force is applied to it. Use caution when handling the flexible cable.</Para>
</item>
<item><Para>The antistatic FPC is connected to the new optical pickup unit. After replacing the optical pickup unit and connecting the flexible cable, cut off the antistatic FPC.</Para>
<Figure><graphic boardno="graphic23" reprowid="170.942mm" reprodep="124.545mm" location="internal"></Figure>
</item>
</seqlist>
</Para>

<!-- Footer -->

<Para>
<link linkend="bex-top">TOP</link>
<nameloc id="bex-top">
<nmlist nametype="entity">
ht623ee
</nmlist>
</nameloc>
<link linkend="bex-previous">PREVIOUS</link>
<nameloc id="bex-previous">
<nmlist nametype="entity">
s1000000000x
</nmlist>
</nameloc>
<link linkend="bex-next">NEXT</link>
<nameloc id="bex-next">
<nmlist nametype="entity">
s1002000000
</nmlist>
</nameloc>
</Para>
</Descriptive>

&hotspot;
</Body>
</ServMan>
</content>
</ServiceMan>
