<!DOCTYPE ServiceMan PUBLIC "-//CEMA//DTD CEMA Service Manual Modular 980431//EN" [
<!ENTITY % nparcon  "(Title? , (SafetyPara | Para | Para1 | Para2 | Para3 | Para4 | Para5 | Example)*)" --<Title>nparcon-- >

<!ELEMENT (Para1 | Para2 | Para3 | Para4 | Para5)  - - (((#PCDATA) | CrossRef | indxflag | change | emphasis | symbol | graphic | Link | subscrpt | supscrpt) | (seqlist | randlist | deflist))+ --<Title>Para-- >

<!ENTITY % mod SYSTEM "module.ent">
%mod;
<!ENTITY % ent SYSTEM "entity.ent">
%ent;
<!ENTITY hotspot SYSTEM "hotspot.ent">
]>
<ServiceMan>
<ManageInfo>
<Ident>
<Category>
</Category>
<Model>SA-HT623EE/SA-HT623GCS/SA-HT623GCU/SA-HT888GCA</Model>
<System>ORDER NO.CHM0408010C3 </System>
<SubSystem>DVD Home Theater Sound System </SubSystem>
<DataType></DataType>
</Ident>
<Status>
<ModuleTitle>s1602010000</ModuleTitle>
<IssueNo issue=1>
<IssueDate day=10 month=Aug year=2004>
<qa>
<Unverif>
</qa>
<ModelName>
<Name>SA-HT623EE/SA-HT623GCS/SA-HT623GCU/SA-HT888GCA</Name>
<SubModelName></SubModelName>
</ModelName>
<PubType pubtype=ServMan>
<Manufacturer></Manufacturer>
<Originator></Originator>
<Author></Author>
<Authorization>
<Language lang=Eng>
</Status>
</ManageInfo>
<content>
<ServMan>
<References><NoRefs></References>

<Body>
<Descriptive>
<Title>16.2.1 Activating Self-Diagnosis Function and Displaying Method</Title>
<Para>
<link linkend="ex-top">TOP</link>
<nameloc id="ex-top">
<nmlist nametype="entity">
ht623ee
</nmlist>
</nameloc>
<link linkend="ex-previous">PREVIOUS</link>
<nameloc id="ex-previous">
<nmlist nametype="entity">
s1602000000
</nmlist>
</nameloc>
<link linkend="ex-next">NEXT</link>
<nameloc id="ex-next">
<nmlist nametype="entity">
s1602020000
</nmlist>
</nameloc>
</Para>
<SubPara><Title>16.2.1.1 Cassette Mechanism Section</Title>
<Para><emphasis>Preparation</emphasis></Para>
<Para><randlist prefix=unorder><item><Para>Music cassette tape with recording tab in either side of A or B.</Para>
</item>
<item><Para>Music cassette tape with recording tab in both side of A and B.</Para>
</item>
</randlist>
</Para>
<Para><emphasis>Note</emphasis></Para>
<Para>Use the tape (30 minutes or more), and play near a center.</Para>
<Para><emphasis>Procedure</emphasis></Para>
<Para><seqlist><item><Para>Turn on the power.</Para>
</item>
<item><Para>Select TAPE mode.</Para>
<Para>With no tape loaded in the unit, press and hold down the FF <graphic boardno="graphic114" reprowid="10.838mm" reprodep="7.451mm" location="internal">button for at least two seconds, and press the <graphic boardno="graphic116" reprowid="10.245mm" reprodep="7.196mm" location="internal">button forat least two seconds simultaneously in order to display &ldquo;T___________TAPE&rdquo;.</Para>
</item>
<item><Para>Load a music cassette tape with the recording tab on the left side removed.</Para>
</item>
<item><Para>Press the FF <graphic boardno="graphic114" reprowid="10.837mm" reprodep="7.451mm" location="internal">button. </Para>
<Para>(FF operation is executed for two seconds, and then stop.)</Para>
</item>
<item><Para>Load a music cassette tape with the recording tab on the right side removed.</Para>
</item>
<item><Para>Press the REW <graphic boardno="graphic113" reprowid="10.245mm" reprodep="7.196mm" location="internal">button. </Para>
<Para>(REW operation is executed for two seconds, and then stop.)</Para>
</item>
<item><Para>Load a music cassette tape (&ast;1) with both recording tabs intact.</Para>
</item>
<item><Para>Press the <graphic boardno="graphic116" reprowid="10.245mm" reprodep="7.196mm" location="internal">button. </Para>
<Para>(TPS operation is executed.)</Para>
</item>
<item><Para>Press the REC <graphic boardno="graphic117" reprowid="10.245mm" reprodep="7.196mm" location="internal"> button. </Para>
<Para>(REC operation is not executed.)</Para>
</item>
<item><Para>Press the <graphic boardno="graphic106" reprowid="7.281mm" reprodep="7.281mm" location="internal">button. </Para>
<Para>If an error is defected, the result of self diagnosis is displayed.</Para>
<Para>(Ex.: T T01) (See table below)</Para>
</item>
</seqlist>
</Para>
<Para>If several errors are detected, press the STOP button to display each.</Para>
<Para><emphasis>Note</emphasis></Para>
<Para><randlist prefix=unorder><item><Para>(&ast;1): TPS (search of music) should not use the following music tapes, in order to use the silent (blank) portion between music.</Para>
<Para>Between music is 4 or less seconds. &sol; Silent part and especially low level are long in music (Ex.: classic etc.).&sol; Recorded by fade-in and fade-out.</Para>
</item>
</randlist>
</Para>
<Figure><graphic boardno="graphic118" reprowid="72.729mm" reprodep="43.688mm" location="internal"></Figure>
</SubPara>
<SubPara><Title>16.2.1.2 DVD&sol;CD Mechanism section</Title>
<Para><seqlist><item><Para>Turn on the power.</Para>
</item>
<item><Para>Select DVD&sol;CD mode. With no DVD&sol;CD inserted in the unit, press and hold down the<graphic boardno="graphic106" reprowid="7.197mm" reprodep="7.197mm" location="internal">button for at least two seconds, and press the F_SKIP<graphic boardno="graphic110" reprowid="10.245mm" reprodep="7.197mm" location="internal">button for at least two seconds simultaneously in order to display &ldquo;T___________DVD&rdquo;. </Para>
<Para><emphasis></emphasis></Para>
</item>
<item><Para>Press the<graphic boardno="graphic106" reprowid="7.197mm" reprodep="7.197mm" location="internal">button. If a memorized error is detected, the result of self diagnosis is displayed. (Ex.: T H15)(See table below) <BR>If several errors are detected, press the<graphic boardno="graphic106" reprowid="7.197mm" reprodep="7.197mm" location="internal">button to display each.</Para>
</item>
</seqlist>
</Para>
<Figure><graphic boardno="graphic119" reprowid="75.861mm" reprodep="32.089mm" location="internal"></Figure>
</SubPara>

<!-- Footer -->

<Para>
<link linkend="bex-top">TOP</link>
<nameloc id="bex-top">
<nmlist nametype="entity">
ht623ee
</nmlist>
</nameloc>
<link linkend="bex-previous">PREVIOUS</link>
<nameloc id="bex-previous">
<nmlist nametype="entity">
s1602000000
</nmlist>
</nameloc>
<link linkend="bex-next">NEXT</link>
<nameloc id="bex-next">
<nmlist nametype="entity">
s1602020000
</nmlist>
</nameloc>
</Para>
</Descriptive>

&hotspot;
</Body>
</ServMan>
</content>
</ServiceMan>
