<!DOCTYPE ServiceMan PUBLIC "-//CEMA//DTD CEMA Service Manual Modular 980431//EN" [
<!ENTITY % nparcon  "(Title? , (SafetyPara | Para | Para1 | Para2 | Para3 | Para4 | Para5 | Example)*)" --<Title>nparcon-- >

<!ELEMENT (Para1 | Para2 | Para3 | Para4 | Para5)  - - (((#PCDATA) | CrossRef | indxflag | change | emphasis | symbol | graphic | Link | subscrpt | supscrpt) | (seqlist | randlist | deflist))+ --<Title>Para-- >

<!ENTITY % mod SYSTEM "module.ent">
%mod;
<!ENTITY % ent SYSTEM "entity.ent">
%ent;
<!ENTITY hotspot SYSTEM "hotspot.ent">
]>
<ServiceMan>
<ManageInfo>
<Ident>
<Category>
</Category>
<Model>SA-HT623EE/SA-HT623GCS/SA-HT623GCU/SA-HT888GCA</Model>
<System>ORDER NO.CHM0408010C3 </System>
<SubSystem>DVD Home Theater Sound System </SubSystem>
<DataType></DataType>
</Ident>
<Status>
<ModuleTitle>s2801000000</ModuleTitle>
<IssueNo issue=1>
<IssueDate day=10 month=Aug year=2004>
<qa>
<Unverif>
</qa>
<ModelName>
<Name>SA-HT623EE/SA-HT623GCS/SA-HT623GCU/SA-HT888GCA</Name>
<SubModelName></SubModelName>
</ModelName>
<PubType pubtype=ServMan>
<Manufacturer></Manufacturer>
<Originator></Originator>
<Author></Author>
<Authorization>
<Language lang=Eng>
</Status>
</ManageInfo>
<content>
<ServMan>
<References><NoRefs></References>

<Body>
<Descriptive>
<Title>28.1 IC6001 (C2CBJG000488): System control</Title>
<Para>
<link linkend="ex-top">TOP</link>
<nameloc id="ex-top">
<nmlist nametype="entity">
ht623ee
</nmlist>
</nameloc>
<link linkend="ex-previous">PREVIOUS</link>
<nameloc id="ex-previous">
<nmlist nametype="entity">
s2800000000x
</nmlist>
</nameloc>
<link linkend="ex-next">NEXT</link>
<nameloc id="ex-next">
<nmlist nametype="entity">
s2900000000p
</nmlist>
</nameloc>
</Para>
<Table frame="all" colsep="1" rowsep="1"><tgroup cols="4" colsep="1" rowsep="1"><colspec colnum="1" colname="1" colwidth="0.315in">
<colspec colnum="2" colname="2" colwidth="0.787in">
<colspec colnum="3" colname="3" colwidth="0.315in">
<colspec colnum="4" colname="4" colwidth="2.067in">
<thead><row rowsep="1"><entry colname="1" align="center"><Para>Pin No.</Para>
</entry>
<entry colname="2" align="center"><Para>Terminal Name</Para>
</entry>
<entry colname="3" align="center"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="center"><Para>Function</Para>
</entry>
</row>
</thead>
<tbody><row rowsep="1"><entry colname="1" align="justify"><Para>1</Para>
</entry>
<entry colname="2" align="justify"><Para>TRY_OPEN</Para>
</entry>
<entry colname="3" align="center"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>Loading mechanism open switch signal input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>2</Para>
</entry>
<entry colname="2" align="justify"><Para>TRY_CLOSE</Para>
</entry>
<entry colname="3" align="center"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>Loading mechanism close switch signal input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>3</Para>
</entry>
<entry colname="2" align="justify"><Para>TRAY_DRV1</Para>
</entry>
<entry colname="3" align="center"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>Tray control signal output (1)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>4</Para>
</entry>
<entry colname="2" align="justify"><Para>TRAY_DRV2</Para>
</entry>
<entry colname="3" align="center"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>Tray control signal output (2)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>5</Para>
</entry>
<entry colname="2" align="justify"><Para>TRAY&sol;TRV</Para>
</entry>
<entry colname="3" align="center"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>Tray control signal output (3)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>6</Para>
</entry>
<entry colname="2" align="justify"><Para>TRAY_MUTE</Para>
</entry>
<entry colname="3" align="center"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>Tray control signal output (4)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>7</Para>
</entry>
<entry colname="2" align="justify"><Para>NC</Para>
</entry>
<entry colname="3" align="center"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>Not used, open</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>8</Para>
</entry>
<entry colname="2" align="justify"><Para>BYTE</Para>
</entry>
<entry colname="3" align="center"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>VSS (GND)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>9</Para>
</entry>
<entry colname="2" align="justify"><Para>CNVSS</Para>
</entry>
<entry colname="3" align="center"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>Connected to GND via resistor</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>10</Para>
</entry>
<entry colname="2" align="justify"><Para>NC</Para>
</entry>
<entry colname="3" align="center"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>Not used, open</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>11</Para>
</entry>
<entry colname="2" align="justify"><Para>NC</Para>
</entry>
<entry colname="3" align="center"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>Not used, open</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>12</Para>
</entry>
<entry colname="2" align="justify"><Para>RESET&sol;ISP_RESET</Para>
</entry>
<entry colname="3" align="center"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>System reset signal input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>13</Para>
</entry>
<entry colname="2" align="justify"><Para>XOUT</Para>
</entry>
<entry colname="3" align="center"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>Main clock output (f&equals;8.0MHz)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>14</Para>
</entry>
<entry colname="2" align="justify"><Para>VSS</Para>
</entry>
<entry colname="3" align="center"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>GND</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>15</Para>
</entry>
<entry colname="2" align="justify"><Para>XIN&sol;ISP_XIN</Para>
</entry>
<entry colname="3" align="center"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>Main clock input (10.0MHz)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>16</Para>
</entry>
<entry colname="2" align="justify"><Para>VCC</Para>
</entry>
<entry colname="3" align="center"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>Power supply (&plus;5V)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>17</Para>
</entry>
<entry colname="2" align="justify"><Para>&sol;NMI</Para>
</entry>
<entry colname="3" align="center"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>Connect to VCC, EXTERNAL INTERRUPT I&sol;P</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>18</Para>
</entry>
<entry colname="2" align="justify"><Para>RMT</Para>
</entry>
<entry colname="3" align="center"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>Remocon signal input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>19</Para>
</entry>
<entry colname="2" align="justify"><Para>SYNC</Para>
</entry>
<entry colname="3" align="center"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>AC failure detect input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>20</Para>
</entry>
<entry colname="2" align="justify"><Para>NC</Para>
</entry>
<entry colname="3" align="center"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>Not used, open</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>21</Para>
</entry>
<entry colname="2" align="justify"><Para>TAPE_BP</Para>
</entry>
<entry colname="3" align="center"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>"AM beatproof 1 output (""L"":BP1, ""H"":BP2)"</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>22</Para>
</entry>
<entry colname="2" align="justify"><Para>TAPE_DMT</Para>
</entry>
<entry colname="3" align="center"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>"Deck mute signal output at mechanism transitio (""L"":mute OFF, ""H"":mute ON)"</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>23</Para>
</entry>
<entry colname="2" align="justify"><Para>TAPE_PL_H</Para>
</entry>
<entry colname="3" align="center"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>"Tape plunger control signal output (""L"":OFF, ""H"":ON)"</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>24</Para>
</entry>
<entry colname="2" align="justify"><Para>TAPE_REC_H</Para>
</entry>
<entry colname="3" align="center"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>"Tape recording ""ON"" signal output (""H"":REC)"</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>25</Para>
</entry>
<entry colname="2" align="justify"><Para>TAPE_MOTOR_H</Para>
</entry>
<entry colname="3" align="center"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>"Capstan motor control signal output (""L"":OFF, ""H"":ON)"</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>26</Para>
</entry>
<entry colname="2" align="justify"><Para>TU_CE(PLL_CE)</Para>
</entry>
<entry colname="3" align="center"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>Tuner PLL latch signal output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>27</Para>
</entry>
<entry colname="2" align="justify"><Para>TU_SD(TUNED)</Para>
</entry>
<entry colname="3" align="center"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>Tuner signal detect input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>28</Para>
</entry>
<entry colname="2" align="justify"><Para>TU_DO(STEREO)</Para>
</entry>
<entry colname="3" align="center"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>Tuner DO input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>29</Para>
</entry>
<entry colname="2" align="justify"><Para>TU_CLK(PLL_CK)</Para>
</entry>
<entry colname="3" align="center"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>Tuner PLL clock signal output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>30</Para>
</entry>
<entry colname="2" align="justify"><Para>TU_DIN(PLL_DA)</Para>
</entry>
<entry colname="3" align="center"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>Tuner PLL DI output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>31</Para>
</entry>
<entry colname="2" align="justify"><Para>ISP_TXD</Para>
</entry>
<entry colname="3" align="center"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>Not used</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>32</Para>
</entry>
<entry colname="2" align="justify"><Para>ISP_RXD</Para>
</entry>
<entry colname="3" align="center"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>Not used</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>33</Para>
</entry>
<entry colname="2" align="justify"><Para>ISP_SCLK</Para>
</entry>
<entry colname="3" align="center"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>Not used</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>34</Para>
</entry>
<entry colname="2" align="justify"><Para>ISP_BUSY</Para>
</entry>
<entry colname="3" align="center"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>Not used</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>35</Para>
</entry>
<entry colname="2" align="justify"><Para>DVD_CMD</Para>
</entry>
<entry colname="3" align="center"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>DVD module command signal output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>36</Para>
</entry>
<entry colname="2" align="justify"><Para>DVD_STA</Para>
</entry>
<entry colname="3" align="center"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>DVD module status signal input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>37</Para>
</entry>
<entry colname="2" align="justify"><Para>DVD_CK</Para>
</entry>
<entry colname="3" align="center"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>DVD module clock signal input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>38</Para>
</entry>
<entry colname="2" align="justify"><Para>WIDE1</Para>
</entry>
<entry colname="3" align="center"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>WIDE function control signal output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>39</Para>
</entry>
<entry colname="2" align="justify"><Para>MUT_FRNT</Para>
</entry>
<entry colname="3" align="center"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>FRONT END mute signal output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>40</Para>
</entry>
<entry colname="2" align="justify"><Para>MUTE_C</Para>
</entry>
<entry colname="3" align="center"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para> Mute signal output fro center</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>41</Para>
</entry>
<entry colname="2" align="justify"><Para>ISP_EPM</Para>
</entry>
<entry colname="3" align="center"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>Not used</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>42</Para>
</entry>
<entry colname="2" align="justify"><Para>SUB_MUTE</Para>
</entry>
<entry colname="3" align="center"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>Mute signal output for subwoofer</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>43</Para>
</entry>
<entry colname="2" align="justify"><Para>HP_MUTE</Para>
</entry>
<entry colname="3" align="center"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>Mute signal output for headphone</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>44</Para>
</entry>
<entry colname="2" align="justify"><Para>DVD_MUTE</Para>
</entry>
<entry colname="3" align="center"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>Mute signal input for DVD module</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>45</Para>
</entry>
<entry colname="2" align="justify"><Para>NC</Para>
</entry>
<entry colname="3" align="center"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>Not used, open</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>46</Para>
</entry>
<entry colname="2" align="justify"><Para>ISP_CE</Para>
</entry>
<entry colname="3" align="center"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>Not used</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>47</Para>
</entry>
<entry colname="2" align="justify"><Para>MUTE_L&sol;MUTE_REC</Para>
</entry>
<entry colname="3" align="center"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>Mute signal output for line output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>48</Para>
</entry>
<entry colname="2" align="justify"><Para>VOL_DA</Para>
</entry>
<entry colname="3" align="center"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>6ch VOL.ASP data signal output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>49</Para>
</entry>
<entry colname="2" align="justify"><Para>VOL_CK</Para>
</entry>
<entry colname="3" align="center"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>6ch VOL.ASP clock signal output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>50</Para>
</entry>
<entry colname="2" align="justify"><Para>MUTE_S</Para>
</entry>
<entry colname="3" align="center"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>Mute signal output for Surround</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>51</Para>
</entry>
<entry colname="2" align="justify"><Para>MIC_MUTE</Para>
</entry>
<entry colname="3" align="center"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>Mute signal output for mic muting circuit</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>52</Para>
</entry>
<entry colname="2" align="justify"><Para>SFC</Para>
</entry>
<entry colname="3" align="center"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>SFC switch signal output during Disco&sol;Live&sol;Hall</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>53</Para>
</entry>
<entry colname="2" align="justify"><Para>SSS_MIX</Para>
</entry>
<entry colname="3" align="center"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>SSS switch signal output during surround function</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>54</Para>
</entry>
<entry colname="2" align="justify"><Para>PARTY</Para>
</entry>
<entry colname="3" align="center"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>PARTY switch signal output during PARTY mode</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>55</Para>
</entry>
<entry colname="2" align="justify"><Para>V_MUTE2</Para>
</entry>
<entry colname="3" align="center"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>Mute signal output for video out (2)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>56</Para>
</entry>
<entry colname="2" align="justify"><Para>V_MUTE1</Para>
</entry>
<entry colname="3" align="center"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>Mute signal output for video out (1)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>57</Para>
</entry>
<entry colname="2" align="justify"><Para>EDA</Para>
</entry>
<entry colname="3" align="center"><Para>I&sol;O</Para>
</entry>
<entry colname="4" align="justify"><Para>EEPROM data signal input&sol;output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>58</Para>
</entry>
<entry colname="2" align="justify"><Para>ECK</Para>
</entry>
<entry colname="3" align="center"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>EEPROM clock signal output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>59</Para>
</entry>
<entry colname="2" align="justify"><Para>ECS</Para>
</entry>
<entry colname="3" align="center"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>EEPROM latch signal output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>60</Para>
</entry>
<entry colname="2" align="justify"><Para>V_MIX&plus;Ctr1</Para>
</entry>
<entry colname="3" align="center"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>Not used, open</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>61</Para>
</entry>
<entry colname="2" align="justify"><Para>V_MUTE3</Para>
</entry>
<entry colname="3" align="center"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>Not used, open</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>62</Para>
</entry>
<entry colname="2" align="justify"><Para>VCC</Para>
</entry>
<entry colname="3" align="center"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>Power supply (&plus;5V)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>63</Para>
</entry>
<entry colname="2" align="justify"><Para>NC</Para>
</entry>
<entry colname="3" align="center"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>Not used, open</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>64</Para>
</entry>
<entry colname="2" align="justify"><Para>VSS</Para>
</entry>
<entry colname="3" align="center"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>GND</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>65</Para>
</entry>
<entry colname="2" align="justify"><Para>NC</Para>
</entry>
<entry colname="3" align="center"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>Not used, open</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>66</Para>
</entry>
<entry colname="2" align="justify"><Para>NC</Para>
</entry>
<entry colname="3" align="center"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>Not used, open</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>67</Para>
</entry>
<entry colname="2" align="justify"><Para>NC</Para>
</entry>
<entry colname="3" align="center"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>Not used, open</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>68</Para>
</entry>
<entry colname="2" align="justify"><Para>DVD_PCNT</Para>
</entry>
<entry colname="3" align="center"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>DVD module power control signal output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>69</Para>
</entry>
<entry colname="2" align="justify"><Para>NC</Para>
</entry>
<entry colname="3" align="center"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>Not used, open</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>70</Para>
</entry>
<entry colname="2" align="justify"><Para>PCONT</Para>
</entry>
<entry colname="3" align="center"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>Power control relay control signal output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>71</Para>
</entry>
<entry colname="2" align="justify"><Para>MUTE_H&sol;MUTE_A</Para>
</entry>
<entry colname="3" align="center"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>Mute signal output for HIC</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>72</Para>
</entry>
<entry colname="2" align="justify"><Para>DC_DET</Para>
</entry>
<entry colname="3" align="center"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>DC detection signal input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>73</Para>
</entry>
<entry colname="2" align="justify"><Para>NC</Para>
</entry>
<entry colname="3" align="center"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>Not used, open</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>74</Para>
</entry>
<entry colname="2" align="justify"><Para>WAKEUP_LED</Para>
</entry>
<entry colname="3" align="center"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>Wake up LED drive signal output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>75</Para>
</entry>
<entry colname="2" align="justify"><Para>JOG_B</Para>
</entry>
<entry colname="3" align="center"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>Volume jog B signal input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>76</Para>
</entry>
<entry colname="2" align="justify"><Para>JOG_A</Para>
</entry>
<entry colname="3" align="center"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>Volume jog A signal input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>77</Para>
</entry>
<entry colname="2" align="justify"><Para>STANDBY_LED</Para>
</entry>
<entry colname="3" align="center"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>Standby LED drive signal output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>78</Para>
</entry>
<entry colname="2" align="justify"><Para>DVD_LED</Para>
</entry>
<entry colname="3" align="center"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>DVD blue LED drive signal output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>79</Para>
</entry>
<entry colname="2" align="justify"><Para>KARA_LED</Para>
</entry>
<entry colname="3" align="center"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>KARA green LED drive signal output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>80</Para>
</entry>
<entry colname="2" align="justify"><Para>MIC_CS</Para>
</entry>
<entry colname="3" align="center"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>Mic IC select enable signal output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>81</Para>
</entry>
<entry colname="2" align="justify"><Para>MIC_CLK</Para>
</entry>
<entry colname="3" align="center"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>Mic 12S clock signal output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>82</Para>
</entry>
<entry colname="2" align="justify"><Para>MIC_DATA</Para>
</entry>
<entry colname="3" align="center"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>Mic 12S data signal output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>83</Para>
</entry>
<entry colname="2" align="justify"><Para>PHONE_SW</Para>
</entry>
<entry colname="3" align="center"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>Phone switch check signal input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>84</Para>
</entry>
<entry colname="2" align="justify"><Para>MIC_SW</Para>
</entry>
<entry colname="3" align="center"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>Mic switch check signal input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>85</Para>
</entry>
<entry colname="2" align="justify"><Para>FLD_CK</Para>
</entry>
<entry colname="3" align="center"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>FL driver clock signal output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>86</Para>
</entry>
<entry colname="2" align="justify"><Para>FLD_DA</Para>
</entry>
<entry colname="3" align="center"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>FL driver data signal output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>87</Para>
</entry>
<entry colname="2" align="justify"><Para>FLD_RST</Para>
</entry>
<entry colname="3" align="center"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>FL driver reset signal output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>88</Para>
</entry>
<entry colname="2" align="justify"><Para>FLD_CS</Para>
</entry>
<entry colname="3" align="center"><Para>O</Para>
</entry>
<entry colname="4" align="justify"><Para>FL driver latch signal output</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>89</Para>
</entry>
<entry colname="2" align="justify"><Para>TAPE_MKIN2</Para>
</entry>
<entry colname="3" align="center"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>Deck AD signal input (2)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>90</Para>
</entry>
<entry colname="2" align="justify"><Para>TAPE_MKIN1</Para>
</entry>
<entry colname="3" align="center"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>Deck AD signal input (1)</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>91</Para>
</entry>
<entry colname="2" align="justify"><Para>KEY2</Para>
</entry>
<entry colname="3" align="center"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>Key 2 line input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>92</Para>
</entry>
<entry colname="2" align="justify"><Para>MIC_VOL</Para>
</entry>
<entry colname="3" align="center"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>Mic volume analog voltage signal input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>93</Para>
</entry>
<entry colname="2" align="justify"><Para>DES3</Para>
</entry>
<entry colname="3" align="center"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>DVD region setting signal input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>94</Para>
</entry>
<entry colname="2" align="justify"><Para>DES2</Para>
</entry>
<entry colname="3" align="center"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>DVD (speaker region) region setting signal input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>95</Para>
</entry>
<entry colname="2" align="justify"><Para>DES1</Para>
</entry>
<entry colname="3" align="center"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>Tuner region setting signal input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>96</Para>
</entry>
<entry colname="2" align="justify"><Para>AVSS(VSS)</Para>
</entry>
<entry colname="3" align="center"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>Analog power supply</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>97</Para>
</entry>
<entry colname="2" align="justify"><Para>KEY1</Para>
</entry>
<entry colname="3" align="center"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>Key 1 line input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>98</Para>
</entry>
<entry colname="2" align="justify"><Para>VREF(VCC)</Para>
</entry>
<entry colname="3" align="center"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>Reference voltage input</Para>
</entry>
</row>
<row rowsep="1"><entry colname="1" align="justify"><Para>99</Para>
</entry>
<entry colname="2" align="justify"><Para>AVCC(VCC)</Para>
</entry>
<entry colname="3" align="center"><Para>-</Para>
</entry>
<entry colname="4" align="justify"><Para>Analog power supply</Para>
</entry>
</row>
<row rowsep="0"><entry colname="1" align="justify"><Para>100</Para>
</entry>
<entry colname="2" align="justify"><Para>TAPE_CRO2</Para>
</entry>
<entry colname="3" align="center"><Para>I</Para>
</entry>
<entry colname="4" align="justify"><Para>CrO2 tape detect signal input</Para>
</entry>
</row>
</tbody>
</tgroup>
</Table>

<!-- Footer -->

<Para>
<link linkend="bex-top">TOP</link>
<nameloc id="bex-top">
<nmlist nametype="entity">
ht623ee
</nmlist>
</nameloc>
<link linkend="bex-previous">PREVIOUS</link>
<nameloc id="bex-previous">
<nmlist nametype="entity">
s2800000000x
</nmlist>
</nameloc>
<link linkend="bex-next">NEXT</link>
<nameloc id="bex-next">
<nmlist nametype="entity">
s2900000000p
</nmlist>
</nameloc>
</Para>
</Descriptive>

&hotspot;
</Body>
</ServMan>
</content>
</ServiceMan>
