<!DOCTYPE ServiceMan PUBLIC "-//CEMA//DTD CEMA Service Manual Modular 980431//EN" [
<!ENTITY % nparcon  "(Title? , (SafetyPara | Para | Para1 | Para2 | Para3 | Para4 | Para5 | Example)*)" --<Title>nparcon-- >

<!ELEMENT (Para1 | Para2 | Para3 | Para4 | Para5)  - - (((#PCDATA) | CrossRef | indxflag | change | emphasis | symbol | graphic | Link | subscrpt | supscrpt) | (seqlist | randlist | deflist))+ --<Title>Para-- >

<!ENTITY % mod SYSTEM "module.ent">
%mod;
<!ENTITY % ent SYSTEM "entity.ent">
%ent;
<!ENTITY hotspot SYSTEM "hotspot.ent">
]>
<ServiceMan>
<ManageInfo>
<Ident>
<Category>
</Category>
<Model>SA-HT623EE/SA-HT623GCS/SA-HT623GCU/SA-HT888GCA</Model>
<System>ORDER NO.CHM0408010C3 </System>
<SubSystem>DVD Home Theater Sound System </SubSystem>
<DataType></DataType>
</Ident>
<Status>
<ModuleTitle>s0201020000</ModuleTitle>
<IssueNo issue=1>
<IssueDate day=10 month=Aug year=2004>
<qa>
<Unverif>
</qa>
<ModelName>
<Name>SA-HT623EE/SA-HT623GCS/SA-HT623GCU/SA-HT888GCA</Name>
<SubModelName></SubModelName>
</ModelName>
<PubType pubtype=ServMan>
<Manufacturer></Manufacturer>
<Originator></Originator>
<Author></Author>
<Authorization>
<Language lang=Eng>
</Status>
</ManageInfo>
<content>
<ServMan>
<References><NoRefs></References>

<Body>
<Descriptive>
<Title>2.1.2 LEAKAGE CURRENT HOT CHECK (See <Link linkend="ex-BEHGGCIJ">Figure 1</Link>

<nameloc id="ex-BEHGGCIJ">
<nmlist nametype=element docorsub=s0201010000>
BEHGGCIJ
</nmlist>
</nameloc>

       .)</Title>
<Para>
<link linkend="ex-top">TOP</link>
<nameloc id="ex-top">
<nmlist nametype="entity">
ht623ee
</nmlist>
</nameloc>
<link linkend="ex-previous">PREVIOUS</link>
<nameloc id="ex-previous">
<nmlist nametype="entity">
s0201010000
</nmlist>
</nameloc>
<link linkend="ex-next">NEXT</link>
<nameloc id="ex-next">
<nmlist nametype="entity">
s0300000000x
</nmlist>
</nameloc>
</Para>
<Para><seqlist><item><Para>Plug the AC cord directly into the AC outlet. Do not use an isolation transformer for this check.</Para>
</item>
<item><Para>Connect a 1.5k&ohm;, 10 watts resistor, in parallel with a 0.15&micro;F capacitors, between each exposed metallic part on the set and a good earth ground such as a water pipe, as shown in <Link linkend="ex-BEHGGCIJ">Figure 1</Link>
.</Para>
</item>
<item><Para>Use an AC voltmeter, with 1000 ohms&sol;volt or more sensitivity, to measure the potential across the resistor.</Para>
</item>
<item><Para>Check each exposed metallic part, and measure the voltage at each point.</Para>
</item>
<item><Para>Reverse the AC plug in the AC outlet and repeat each of the above measurements.</Para>
</item>
<item><Para>The potential at any point should not exceed 0.75 volts RMS. A leakage current tester (Simpson Model 229 or equivalent) may be used to make the hot checks, leakage current must not exceed 1&sol;2 milliamp. In case a measurement is outsideof the limits specified, there is a possibility of a shock hazard, and the equipment should be repaired and rechecked before it is returned to the customer.</Para>
<Para></Para>
<Para></Para>
</item>
</seqlist>
</Para>

<!-- Footer -->

<Para>
<link linkend="bex-top">TOP</link>
<nameloc id="bex-top">
<nmlist nametype="entity">
ht623ee
</nmlist>
</nameloc>
<link linkend="bex-previous">PREVIOUS</link>
<nameloc id="bex-previous">
<nmlist nametype="entity">
s0201010000
</nmlist>
</nameloc>
<link linkend="bex-next">NEXT</link>
<nameloc id="bex-next">
<nmlist nametype="entity">
s0300000000x
</nmlist>
</nameloc>
</Para>
</Descriptive>

&hotspot;
</Body>
</ServMan>
</content>
</ServiceMan>
