<?xml version="1.0" encoding="utf-8"?>
<?xml-stylesheet href="DSD0405014C8.css" type="text/css"?>
<!-- DC Version =\\\\\\\\ "(unknown).0.0.1" -->
<!-- Character entity set. Typical invocation:
     <!ENTITY % ISOnum PUBLIC
       "ISO 8879-1986//ENTITIES Numeric and Special Graphic//EN">
     %ISOnum;
-->
<svctechdoc lang="english" type="svc" xmlns:html="http://www.w3.org/Profiles/XHTML-transitional">
<html:script language="JavaScript" src="script.js"></html:script>
<html:script language="JavaScript" src="tree.js"></html:script>
<html:body onload="dgfFsetClose();setScroll();">
<other>
<ttl><html:a name="TITLE3">3 Prevention of Electrostatic Discharge (ESD) to Electrostatic Sensitive (ES) Devices </html:a>
</ttl>
<p>Some semiconductor (solid state) devices can be damaged easily by static electricity. Such components commonly are called Electrostatic Sensitive (ES) Devices. Examples of typical ES devices are integrated circuits and some field-effect transistor-sandsemiconductor
"chip" components. The following techniques should be used to help reduce the incidence of component damage caused by electrostatic discharge (ESD).</p>
<ol>
<li>
<p>Immediately before handling any semiconductor component or semiconductor-equipped assembly, drain off any ESD on your body by touching a known earth ground. Alternatively, obtain and wear a commercially available discharging ESD wrist strap, whichshould
be removed for potential shock reasons prior to applying power to the unit under test.</p>
</li>
<li>
<p>After removing an electrical assembly equipped with ES devices, place the assembly on a conductive surface such as aluminum foil, to prevent electrostatic charge buildup or exposure of the assembly.
</p>
</li>
<li>
<p>Use only a grounded-tip soldering iron to solder or unsolder ES devices.
</p>
</li>
<li>
<p>Use only an anti-static solder removal device. Some solder removal devices not classified as "anti-static (ESD protected)" can generate electrical charge sufficient to damage ES devices.
</p>
</li>
<li>
<p>Do not use freon-propelled chemicals. These can generate electrical charges sufficient to damage ES devices.
</p>
</li>
<li>
<p>Do not remove a replacement ES device from its protective package until immediately before you are ready to install it. (Most replacement ES devices are packaged with leads electrically shorted together by conductive foam, aluminum foil or comparableconductive
material).</p>
</li>
<li>
<p>Immediately before removing the protective material from the leads of a replacement ES device, touch the protective material to the chassis or circuit assembly into which the device will be installed.
</p>
<caution>
<ttl>Caution
</ttl>
<p>Be sure no power is applied to the chassis or circuit, and observe all other safety precautions.
</p>
</caution>
</li>
<li>
<p>Minimize bodily motions when handling unpackaged replacement ES devices. (Otherwise hamless motion such as the brushing together of your clothes fabric or the lifting of your foot from a carpeted floor can generate static electricity sufficientto damage
an ES device).</p>
</li>
</ol>
<fig>
<graphic loc="graphic5" sizex="163.746mm" sizey="28.534mm"><html:img src="notice.png" border="0"></html:img>
</graphic>
</fig>
</other>
</html:body>
</svctechdoc>
