<?xml version="1.0" encoding="utf-8"?>
<?xml-stylesheet href="DSD0405014C8.css" type="text/css"?>
<!-- DC Version =\\\\\\\\ "(unknown).0.0.1" -->
<!-- Character entity set. Typical invocation:
     <!ENTITY % ISOnum PUBLIC
       "ISO 8879-1986//ENTITIES Numeric and Special Graphic//EN">
     %ISOnum;
-->
<svctechdoc lang="english" type="svc" xmlns:html="http://www.w3.org/Profiles/XHTML-transitional">
<html:script language="JavaScript" src="script.js"></html:script>
<html:script language="JavaScript" src="tree.js"></html:script>
<html:body onload="dgfFsetClose();setScroll();">
<other>
<ttl><html:a name="TITLE16">16 Abbreviations </html:a>
</ttl>
<table frame="all" colsep="1" rowsep="1"><html:table frame="all" rules="all" >
<tgroup cols="3" colsep="1" rowsep="1">
<colspec colnum="1" colname="1" colwidth="0.394in">
</colspec>
<colspec colnum="2" colname="2" colwidth="0.787in">
</colspec>
<colspec colnum="3" colname="3" colwidth="2.165in">
</colspec>
<thead>
<row rowsep="1"><html:tr>
<entry namest="1" nameend="2" align="center"><html:td valign="top" align="center" colspan="2" rowspan="1">
<p>INITIAL&#47;LOGO
</p>
</html:td></entry>
<entry colname="3" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>ABBREVIATIONS
</p>
</html:td></entry>
</html:tr></row>
</thead>
<tbody>
<row rowsep="1"><html:tr>
<entry colname="1" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>A
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>A0~UP
</p> 
<p>ACLK
</p> 
<p>AD0~UP
</p> 
<p>ADATA
</p> 
<p>ALE
</p> 
<p>AMUTE
</p> 
<p>AREQ
</p> 
<p>ARF
</p> 
<p>ASI
</p> 
<p>ASO
</p> 
<p>ASYNC
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>ADDRESS
</p> 
<p>AUDIO CLOCK
</p> 
<p>ADDRESS BUS
</p> 
<p>AUDIO PES PACKET DATA
</p> 
<p>ADDRESS LATCH ENABLE
</p> 
<p>AUDIO MUTE
</p> 
<p>AUDIO PES PACKET REQUEST
</p> 
<p>AUDIO RF
</p> 
<p>SERVO AMP INVERTED INPUT
</p> 
<p>SERVO
AMPOUTPUT</p> 
<p>AUDIO WORD DISTINCTION SYNC
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>B
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>BCK
</p> 
<p>BCKIN
</p> 
<p>BDO
</p> 
<p>BLKCK
</p> 
<p>BOTTOM
</p> 
<p>BYP
</p> 
<p>BYTCK
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>BIT CLOCK (PCM)
</p> 
<p>BIT CLOCK INPUT
</p> 
<p>BLACK DROP OUT
</p> 
<p>SUB CODE BLOCK CLOCK
</p> 
<p>CAP. FOR BOTTOM HOLD
</p> 
<p>BYPATH
</p> 
<p>BYTE CLOCK
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>C
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>CAV
</p> 
<p>CBDO
</p> 
<p>CD
</p> 
<p>CDSCK
</p> 
<p>CDSRDATA
</p> 
<p>CDRF
</p> 
<p>CDV
</p> 
<p>CHNDATA
</p> 
<p>CKSL
</p> 
<p>CLV
</p> 
<p>COFTR
</p> 
<p>CPA
</p> 
<p>CPCS
</p> 
<p>CPDT
</p> 
<p>CPUADR
</p> 
<p>CPUADT
</p> 
<p>CPUIRQ
</p> 
<p>CPRD
</p> 
<p>CPWR
</p> 
<p>CS
</p> 
<p>CSYNCIN
</p> 
<p>CSYNCOUT
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>CONSTANT ANGULAR VELOCITY
</p> 
<p>CAP. BLACK DROP OUT
</p> 
<p>COMPACT DISC
</p> 
<p>CD SERIAL DATA CLOCK
</p> 
<p>CD SERIAL DATA
</p> 
<p>CD RF (EFM) SIGNAL
</p> 
<p>COMPACT DISC-VIDEO
</p> 
<p>CHANNEL DATA
</p> 
<p>SYSTEM
CLOCKSELECT</p> 
<p>CONSTANT LINEAR VELOCITY
</p> 
<p>CAP. OFF TRACK
</p> 
<p>CPU ADDRESS
</p> 
<p>CPU CHIP SELECT
</p> 
<p>CPU DATA
</p> 
<p>CPU ADDRESS LATCH
</p> 
<p>CPU ADDRESS DATA BUS
</p> 
<p>CPU INTERRUPT REQUEST
</p> 
<p>CPU READ ENABLE
</p> 
<p>CPU WRITE ENABLE
</p> 
<p>CHIPSELECT
</p> 
<p>COMPOSITE
SYNC IN</p> 
<p>COMPOSITE SYNC OUT
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="0"><html:tr>
<entry colname="1" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>D
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>DACCK
</p> 
<p>DEEMP
</p> 
<p>DEMPH
</p> 
<p>DIG0~UP
</p> 
<p>DIN
</p> 
<p>DMSRCK
</p> 
<p>DMUTE
</p> 
<p>DO
</p> 
<p>DOUT0~UP
</p> 
<p>DRF
</p> 
<p>DRPOUT
</p> 
<p>DREQ
</p> 
<p>DRESP
</p> 
<p>DSC
</p> 
<p>DSLF
</p> 
<p>DVD
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>D&#47;A CONVERTER CLOCK
</p> 
<p>DEEMPHASIS BIT ON&#47;OFF
</p> 
<p>DEEMPHASIS SWITCHING
</p> 
<p>FL DIGIT OUTPUT
</p> 
<p>DATA INPUT
</p> 
<p>DM SERIAL DATA READ CLOCK
</p> 
<p>DIGITAL MUTE CONTROL
</p> 
<p>DROP
OUT</p> 
<p>DATAOUTPUT
</p> 
<p>DATA SLICE RF (BIAS)
</p> 
<p>DROP OUT SIGNAL
</p> 
<p>DATA REQUEST
</p> 
<p>DATA RESPONSE
</p> 
<p>DIGITAL SERVO CONTROLLER
</p> 
<p>DATA SLICE LOOP FILTER
</p> 
<p>DIGITAL VIDEO DISC
</p>
</html:td></entry>
</html:tr></row>
</tbody>
</tgroup>
</html:table></table>
<table frame="all" colsep="1" rowsep="1" newcol="1"><html:table frame="all" rules="all" >
<tgroup cols="3" colsep="1" rowsep="1">
<colspec colnum="1" colname="1" colwidth="0.394in">
</colspec>
<colspec colnum="2" colname="2" colwidth="0.787in">
</colspec>
<colspec colnum="3" colname="3" colwidth="2.165in">
</colspec>
<thead>
<row rowsep="1"><html:tr>
<entry namest="1" nameend="2" align="center"><html:td valign="top" align="center" colspan="2" rowspan="1">
<p>INITIAL&#47;LOGO
</p>
</html:td></entry>
<entry colname="3" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>ABBREVIATIONS
</p>
</html:td></entry>
</html:tr></row>
</thead>
<tbody>
<row rowsep="1"><html:tr>
<entry colname="1" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>E
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>EC
</p> 
<p>ECR
</p> 
<p>
</p> 
<p>ENCSEL
</p> 
<p>ETMCLK
</p> 
<p>ETSCLK
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>ERROR TORQUE CONTROL
</p> 
<p>ERROR TORQUE CONTROL REFERENCE
</p> 
<p>ENCODER SELECT
</p> 
<p>EXTERNAL M CLOCK (81MHz&#47;40.5MHz)
</p> 
<p> EXTERNAL S CLOCK (54MHz)
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>F
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>FBAL
</p> 
<p>FCLK
</p> 
<p>FE
</p> 
<p>FFI
</p> 
<p>FEO
</p> 
<p>FG
</p> 
<p>FSC
</p> 
<p>FSCK
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>FOCUS BALANCE
</p> 
<p>FRAME CLOCK
</p> 
<p>FOCUS ERROR
</p> 
<p>FOCUS ERROR AMP INVERTED INPUT
</p> 
<p>FOCUS ERROR AMP OUTPUT
</p> 
<p>FREQUENCY GENERATOR
</p> 
<p>FREQUENCY SUB CARRIER
</p> 
<p>FS (384 OVER SAMPLING)
CLOCK</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>G
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>GND
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>COMMON GROUNDING (EARTH)
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>H
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>HA0~UP
</p> 
<p>HD0~UP
</p> 
<p>HINT
</p> 
<p>HRXW
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>HOST ADDRESS
</p> 
<p>HOST DATA
</p> 
<p>HOST INTERRUPT
</p> 
<p>HOST READ&#47;WRITE
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>I
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>IECOUT
</p> 
<p>IPFRAG
</p> 
<p>IREF
</p> 
<p>ISEL
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>IEC958 FORMAT DATA OUTPUT
</p> 
<p>INTERPOLATION FLAG
</p> 
<p>I (CURRENT) REFERENCE
</p> 
<p>INTERFACE MODE SELECT
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>L
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>LDON
</p> 
<p>LPC
</p> 
<p>LRCK
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>LASER DIODE CONTROL
</p> 
<p>LASER POWER CONTROL
</p> 
<p>L CH&#47;R CH DISTINCTION CLOCK
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>M
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>MA0~UP
</p> 
<p>MCK
</p> 
<p>MCKI
</p> 
<p>MCLK
</p> 
<p>MDATA
</p> 
<p>MDQ0~UP
</p> 
<p>MDQM
</p> 
<p>MLD
</p> 
<p>MPEG
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>MEMORY ADDRESS
</p> 
<p>MEMORY CLOCK
</p> 
<p>MEMORY CLOCK INPUT
</p> 
<p>MEMORY SERIAL COMMAND CLOCK
</p> 
<p>MEMORY SERIAL COMMAND DATA
</p> 
<p>MEMORY DATA INPUT&#47;OUTPUT
</p> 
<p>MEMORY DATA I&#47;O MASK
</p> 
<p>MEMORYSERIAL
COMMAND LOAD</p> 
<p>MOVING PICTURE EXPERTS GROUP
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>O
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>ODC
</p> 
<p>OFTR
</p> 
<p>OSCI
</p> 
<p>OSCO
</p> 
<p>OSD
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>OPTICAL DISC CONTROLLER
</p> 
<p>OFF TRACKING
</p> 
<p>OSCILLATOR INPUT
</p> 
<p>OSCILLATOR OUTPUT
</p> 
<p>ON SCREEN DISPLAY
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="0"><html:tr>
<entry colname="1" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>P
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>P1~UP
</p> 
<p>PCD
</p> 
<p>PCK
</p> 
<p>PDVD
</p> 
<p>PEAK
</p> 
<p>PLLCLK
<br><html:br></html:br>
</br>PLLOK
</p> 
<p>PWMCTL
</p> 
<p>PWMDA
</p> 
<p>PWMOA, B
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>PORT
</p> 
<p>CD TRACKING PHASE DIFFERENCE
</p> 
<p>PLL CLOCK
</p> 
<p>DVD TRACKING PHASE DIFFERENCE
</p> 
<p>CAP. FOR PEAK HOLD
</p> 
<p>CHANNEL PLL CLOCK
</p> 
<p>PLL LOCK
</p> 
<p>PWM OUTPUT CONTROL
</p> 
<p>PULSE WAVE
MOTOR DRIVEA</p> 
<p>PULSE WAVE MOTOR OUT A, B
</p>
</html:td></entry>
</html:tr></row>
</tbody>
</tgroup>
</html:table></table>
<table frame="all" colsep="1" rowsep="1" newpage="1"><html:table frame="all" rules="all" >
<tgroup cols="3" colsep="1" rowsep="1">
<colspec colnum="1" colname="1" colwidth="0.394in">
</colspec>
<colspec colnum="2" colname="2" colwidth="0.787in">
</colspec>
<colspec colnum="3" colname="3" colwidth="2.165in">
</colspec>
<thead>
<row rowsep="1"><html:tr>
<entry namest="1" nameend="2" align="center"><html:td valign="top" align="center" colspan="2" rowspan="1">
<p>INITIAL&#47;LOGO
</p>
</html:td></entry>
<entry colname="3" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>ABBREVIATIONS
</p>
</html:td></entry>
</html:tr></row>
</thead>
<tbody>
<row rowsep="1"><html:tr>
<entry colname="1" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>R
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>RE
</p> 
<p>RFENV
</p> 
<p>RFO
</p> 
<p>RS
</p> 
<p>RSEL
</p> 
<p>RST
</p> 
<p>RSV
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>READ ENABLE
</p> 
<p>RF ENVELOPE
</p> 
<p>RF PHASE DIFFERENCE OUTPUT
</p> 
<p>(CD-ROM) REGISTER SELECT
</p> 
<p>RF POLARITY SELECT
</p> 
<p>RESET
</p> 
<p>RESERVE
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>S
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>SBI0, 1
</p> 
<p>SBO0
</p> 
<p>SBT0, 1
</p> 
<p>SCK
</p> 
<p>SCKR
</p> 
<p>SCL
</p> 
<p>SCLK
</p> 
<p>SDA
</p> 
<p>SEG0~UP
</p> 
<p>SELCLK
</p> 
<p>SEN
</p> 
<p>SIN1, 2
</p> 
<p>SOUT1, 2
</p> 
<p>SPDI
</p> 
<p>SPDO
</p> 
<p>SPEN
</p> 
<p>SPRCLK
</p> 
<p>SPWCLK
</p> 
<p>SQCK
</p> 
<p>SQCX
</p> 
<p>SRDATA
</p> 
<p>SRMADR
</p> 
<p>SRMDT0~7
</p> 
<p>SS
</p> 
<p>STAT
</p> 
<p>STCLK
</p> 
<p>STD0~UP
</p> 
<p>STENABLE
</p> 
<p>STSEL
</p> 
<p>STVALID
</p> 
<p>SUBC
</p> 
<p>SBCK
</p> 
<p>SUBQ
</p> 
<p>SYSCLK
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>SERIAL DATA INPUT
</p> 
<p>SERIAL DATA OUTPUT
</p> 
<p>SERIAL CLOCK
</p> 
<p>SERIAL DATA CLOCK
</p> 
<p>AUDIO SERIAL CLOCK RECEIVER
</p> 
<p>SERIAL CLOCK
</p> 
<p>SERIAL CLOCK
</p> 
<p>SERIAL DATA
</p> 
<p>FL SEGMENT OUTPUT
</p> 
<p>SELECTCLOCK
</p> 
<p>SERIAL
PORT ENABLE</p> 
<p>SERIAL DATA IN
</p> 
<p>SERIAL DATA OUT
</p> 
<p>SERIAL PORT DATA INPUT
</p> 
<p>SERIAL PORT DATA OUTPUT
</p> 
<p>SERIAL PORT R&#47;W ENABLE
</p> 
<p>SERIAL PORT READ CLOCK
</p> 
<p>SERIAL PORT WRITE CLOCK
</p> 
<p>SUB CODE Q CLOCK
</p> 
<p>SUBCODE
Q DATA READ CLOCK</p> 
<p>SERIAL DATA
</p> 
<p>SRAM ADDRESS BUS
</p> 
<p>SRAM DATA BUS 0~7
</p> 
<p>START&#47;STOP
</p> 
<p>STATUS
</p> 
<p>STREAM DATA CLOCK
</p> 
<p>STREAM DATA
</p> 
<p>STREAM DATA INPUT ENABLE
</p> 
<p>STREAM DATA POLARITY SELECT
</p> 
<p>STREAM
DATAVALIDITY</p> 
<p>SUB CODE SERIAL
</p> 
<p>SUB CODE CLOCK
</p> 
<p>SUB CODE Q DATA
</p> 
<p>SYSTEM CLOCK
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="0"><html:tr>
<entry colname="1" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>T
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>TE
</p> 
<p>TIBAL
</p> 
<p>TID
</p> 
<p>TIN
</p> 
<p>TIP
</p> 
<p>TIS
</p> 
<p>TPSN
</p> 
<p>TPSO
</p> 
<p>TPSP
</p> 
<p>TRCRS
</p> 
<p>TRON
</p> 
<p>TRSON
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>TRACKING ERROR
</p> 
<p>BALANCE CONTROL
</p> 
<p>BALANCE OUTPUT 1
</p> 
<p>BALANCE INPUT
</p> 
<p>BALANCE INPUT
</p> 
<p>BALANCE OUTPUT 2
</p> 
<p>OP AMP INPUT
</p> 
<p>OP AMP OUTPUT
</p> 
<p>OP AMP INVERTED INPUT
</p> 
<p>TRACK
CROSSSIGNAL</p> 
<p>TRACKING ON
</p> 
<p>TRAVERSE SERVO ON
</p>
</html:td></entry>
</html:tr></row>
</tbody>
</tgroup>
</html:table></table>
<table frame="all" colsep="1" rowsep="1" newcol="1"><html:table frame="all" rules="all" >
<tgroup cols="3" colsep="1" rowsep="1">
<colspec colnum="1" colname="1" colwidth="0.394in">
</colspec>
<colspec colnum="2" colname="2" colwidth="0.787in">
</colspec>
<colspec colnum="3" colname="3" colwidth="2.165in">
</colspec>
<thead>
<row rowsep="1"><html:tr>
<entry namest="1" nameend="2" align="center"><html:td valign="top" align="center" colspan="2" rowspan="1">
<p>INITIAL&#47;LOGO
</p>
</html:td></entry>
<entry colname="3" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>ABBREVIATIONS
</p>
</html:td></entry>
</html:tr></row>
</thead>
<tbody>
<row rowsep="1"><html:tr>
<entry colname="1" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>V
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>VBLANK
</p> 
<p>VCC
</p> 
<p>
</p> 
<p>VCDCONT
</p> 
<p>
</p> 
<p>VDD
</p> 
<p>VFB
</p> 
<p>VREF
</p> 
<p>VSS
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>V BLANKING
</p> 
<p>COLLECTOR POWER SUPPLY 
</p> 
<p>VOLTAGE
</p> 
<p>VIDEO CD CONTROL (TRACKING 
</p> 
<p>BALANCE)
</p> 
<p>DRAIN POWER SUPPLY VOLTAGE
</p> 
<p>VIDEO FEED BACK
</p> 
<p>VOLTAGE REFERENCE
</p> 
<p>SOURCE POWER
SUPPLYVOLTAGE</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>W
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>WAIT
</p> 
<p>WDCK
</p> 
<p>WEH
</p> 
<p>WSR
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>BUS CYCLE WAIT
</p> 
<p>WORD CLOCK
</p> 
<p>WRITE ENABLE HIGH
</p> 
<p>WORD SELECT RECEIVER
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="0"><html:tr>
<entry colname="1" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>X
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>X
</p> 
<p>XALE
</p> 
<p>XAREQ
</p> 
<p>XCDROM
</p> 
<p>XCS
</p> 
<p>XCSYNC
</p> 
<p>XDS
</p> 
<p>XHSYNCO
</p> 
<p>XHINT
</p> 
<p>XI
</p> 
<p>XINT
</p> 
<p>XMW
</p> 
<p>XO
</p> 
<p>XRE
</p> 
<p>XSRMCE
</p> 
<p>XSRMOE
</p> 
<p>XSRMWE
</p> 
<p>XVCS
</p> 
<p>XVDS
</p> 
<p>XVSYNCO
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>X&#700; TAL
</p> 
<p>X ADDRESS LATCH ENABLE
</p> 
<p>X AUDIO DATA REQUEST
</p> 
<p>X CD ROM CHIP SELECT
</p> 
<p>X CHIP SELECT
</p> 
<p>X COMPOSITE SYNC
</p> 
<p>X DATA STROBE
</p> 
<p>X HORIZONTAL SYNC OUTPUT
</p> 
<p>XH
INTERRUPTREQUEST</p> 
<p>X&#700; TAL OSCILLATOR INPUT
</p> 
<p>X INTERRUPT
</p> 
<p>X MEMORY WRITE ENABLE
</p> 
<p>X&#700; TAL OSCILLATOR OUTPUT
</p> 
<p>X READ ENABLE
</p> 
<p>X SRAM CHIP ENABLE
</p> 
<p>X SRAM OUTPUT ENABLE
</p> 
<p>X SRAM WRITE ENABLE
</p> 
<p>X
V-DEC CHIPSELECT</p> 
<p>X V-DEC CONTROL BUS STROBE
</p> 
<p>X VERTICAL SYNC OUTPUT
</p>
</html:td></entry>
</html:tr></row>
</tbody>
</tgroup>
</html:table></table>
</other>
</html:body>
</svctechdoc>
