<?xml version="1.0" encoding="utf-8"?>
<?xml-stylesheet href="DSD0405014C8.css" type="text/css"?>
<!-- DC Version =\\\\\\\\ "(unknown).0.0.1" -->
<!-- Character entity set. Typical invocation:
     <!ENTITY % ISOnum PUBLIC
       "ISO 8879-1986//ENTITIES Numeric and Special Graphic//EN">
     %ISOnum;
-->
<svctechdoc lang="english" type="svc" xmlns:html="http://www.w3.org/Profiles/XHTML-transitional">
<html:script language="JavaScript" src="script.js"></html:script>
<html:script language="JavaScript" src="tree.js"></html:script>
<html:body onload="dgfFsetClose();setScroll();">
<other>
<ttl><html:a name="TITLE9">9 Self-Diagnosis and Special Mode Setting </html:a>
</ttl>
<ti2 column="3">
<ttl><html:a name="TITLE9_1">9.1 Self-Diagnosis Functions </html:a>
</ttl>
<p>Self-Diagnosis Function provides information for errors to service personnel by &#8220;Self-Diagnosis Display&#8221; when any error has occurred.
</p>
<p>
<emp>U14, H&#42;&#42; and F&#42;&#42; are stored in memory and held.
</emp>
</p>
<p>Display on FL will be cancelled when the power is turned off or AC input is turned off during self-diagnosis display is ON.
</p>
<table frame="all" colsep="1" rowsep="1"><html:table frame="all" rules="all" >
<tgroup cols="5" colsep="1" rowsep="1">
<colspec colnum="1" colname="1" colwidth="0.591in">
</colspec>
<colspec colnum="2" colname="2" colwidth="1.575in">
</colspec>
<colspec colnum="3" colname="3" colwidth="2.283in">
</colspec>
<colspec colnum="4" colname="4" colwidth="1.024in">
</colspec>
<colspec colnum="5" colname="5" colwidth="1.732in">
</colspec>
<thead>
<row rowsep="1"><html:tr>
<entry colname="1" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>Error
</p> 
<p>Code
</p>
</html:td></entry>
<entry colname="2" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>Diagnosis contents
</p>
</html:td></entry>
<entry colname="3" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>Description
</p>
</html:td></entry>
<entry colname="4" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>Monitor Display
</p>
</html:td></entry>
<entry colname="5" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>FL display
</p>
</html:td></entry>
</html:tr></row>
</thead>
<tbody>
<row rowsep="1"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>U12
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Remote control code error
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Display appears when main unit and remote controller codes are not matched.
</p>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>No display
</p>
</html:td></entry>
<entry colname="5" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<fig>
<graphic loc="graphic19" sizex="42.000mm" sizey="10.500mm"><html:img src="re080101.png" border="0"></html:img>
</graphic>
</fig> 
<p>&#8220;&#42;&#8221; is remote controller code of the main unit.
</p> 
<p>Display for 5 seconds.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>U14
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Abnormal inner temperature detected
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Display appears when the drive temperature exceeds 70&#176;C.
</p> 
<p>The power is turned off forcibly.
</p> 
<p>For 30 minutes after this, all key entries are disabled. (Fan motor operates at the highest speedfor
the first 5 minutes. For the remaining 25 minutes, fan motor is also stopped.) The event is saved in memory as well.</p>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>No display
</p>
</html:td></entry>
<entry colname="5" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<fig>
<graphic loc="graphic20" sizex="42.000mm" sizey="10.500mm"><html:img src="re080102.png" border="0"></html:img>
</graphic>
</fig> 
<p>&#8220;U14&#8221; is displayed for 30 minutes.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>U99
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Hang-up
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Displayed when communication error has occurred between Main microprocessor and Timer microprocessor.
</p>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>No display
</p>
</html:td></entry>
<entry colname="5" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<fig>
<graphic loc="graphic21" sizex="42.000mm" sizey="10.500mm"><html:img src="re080103.png" border="0"></html:img>
</graphic>
</fig> 
<p>Displayed is left until the [POWER] key is pressed.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>H01
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Inoperative fan motor
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Display appears when inoperative fan motor is detected after powered on.
</p> 
<p>The power is turned off when detecting.
</p>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>No display
</p>
</html:td></entry>
<entry colname="5" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<fig>
<graphic loc="graphic22" sizex="42.000mm" sizey="10.500mm"><html:img src="re080104.png" border="0"></html:img>
</graphic>
</fig> 
<p>Displayed is left.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>F00
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>No error information
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Initial setting for error code in memory
</p> 
<p>(Error code Initialization is possible with error code initialization and main unit initialization.)
</p>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>No display
</p>
</html:td></entry>
<entry colname="5" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<fig>
<graphic loc="graphic23" sizex="42.000mm" sizey="10.500mm"><html:img src="re080105.png" border="0"></html:img>
</graphic>
</fig> 
<p>Displayed is left.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>F01
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Drive hardware error
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Display appears when drive unit error is detected. The event is saved in memory.
</p>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>No display
</p>
</html:td></entry>
<entry colname="5" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<fig>
<graphic loc="graphic24" sizex="42.000mm" sizey="10.500mm"><html:img src="re080106.png" border="0"></html:img>
</graphic>
</fig> 
<p>Displayed is left.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>F12
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Initialization error when main microprocessor is started up for program recording
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Display appears when initialization error is detected after starting up main microprocessor for program recording. The event is saved in memory.
</p> 
<p>The power is turned off when detecting.
</p>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>No display
</p>
</html:td></entry>
<entry colname="5" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<fig>
<graphic loc="graphic25" sizex="42.000mm" sizey="10.500mm"><html:img src="re080107.png" border="0"></html:img>
</graphic>
</fig> 
<p>Displayed is left.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>UNSUPPORT
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Unsupported disc error
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>&#42;An unsupported format disc was played, although the drive starts normally.
</p> 
<p>&#42;The data format is not supported, although the media type is supported.
</p> 
<p>&#42;Exceptionally incase
of the disc is dirty.</p>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>
<emp>&#8220;This disc is incompatible.&#8221; 
</emp>
</p>
</html:td></entry>
<entry colname="5" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<fig>
<graphic loc="graphic26" sizex="42.000mm" sizey="10.500mm"><html:img src="re080108.png" border="0"></html:img>
</graphic>
</fig> 
<p>Display for 5 seconds.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>NO READ
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Disc read error
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>&#42;A disc is flawed or dirty.
</p> 
<p>&#42;A poor quality failed to start.
</p> 
<p>&#42;The track information could not be read.
</p>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>
<emp>&#8220;Cannot read. Please check the disc.&#8221; 
</emp>
</p>
</html:td></entry>
<entry colname="5" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<fig>
<graphic loc="graphic27" sizex="42.000mm" sizey="10.500mm"><html:img src="re080109.png" border="0"></html:img>
</graphic>
</fig>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>HARD ERR
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Drive error
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>The drive detected a hard error.
</p>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>&#8220; 
<emp>DVD drive
</emp> error.&#8221; 
</p>
</html:td></entry>
<entry colname="5" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Display for 5 seconds.
</p> 
<fig>
<graphic loc="graphic28" sizex="42.000mm" sizey="10.500mm"><html:img src="re080110.png" border="0"></html:img>
</graphic>
</fig>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>SELF CHECK
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Restoration operation
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Since the power cord fell out during a power failure or operation, it is under restoration operation.
</p> 
<p>&#42;It will OK, if a display disappears automatically. If a display does not disappear, thereis the
possibility that defective Digital P.C.B. &#47; RAM drive.</p>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>No display
</p>
</html:td></entry>
<entry colname="5" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<fig>
<graphic loc="graphic29" sizex="42.000mm" sizey="10.500mm"><html:img src="re080111.png" border="0"></html:img>
</graphic>
</fig>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Full Program
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>32 programs are already set.
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>32 programs are already set.
</p>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>No display
</p>
</html:td></entry>
<entry colname="5" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<fig>
<graphic loc="graphic30" sizex="42.000mm" sizey="10.500mm"><html:img src="re080112.png" border="0"></html:img>
</graphic>
</fig>
</html:td></entry>
</html:tr></row>
<row rowsep="0"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>HDD SLEEP
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>In order to extend HDD life, the HDD is in SLEEP (not activated) mode.
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>If there is no disc in the unit, the HDD will go into SLEEP mode after there has been no operation for 30 minutes or longer.
</p> 
<p>
</p> 
<p>&#42;While in SLEEP mode play or recording may not begin rightaway
because the HDD takes time to be re-activated.</p>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>&#8220;HDD SLEEP&#8220; is displayed for 3 seconds.
</p>
</html:td></entry>
<entry colname="5" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<fig>
<graphic loc="graphic31" sizex="42.000mm" sizey="10.500mm"><html:img src="re080113.png" border="0"></html:img>
</graphic>
</fig>
</html:td></entry>
</html:tr></row>
</tbody>
</tgroup>
</html:table></table>
</ti2>
<ti2 column="3">
<ttl><html:a name="TITLE9_2">9.2 Special Modes Setting </html:a>
</ttl>
<table frame="all" colsep="1" rowsep="1"><html:table frame="all" rules="all" >
<tgroup cols="4" colsep="1" rowsep="1">
<colspec colnum="1" colname="1" colwidth="1.299in">
</colspec>
<colspec colnum="2" colname="2" colwidth="2.283in">
</colspec>
<colspec colnum="3" colname="3" colwidth="1.811in">
</colspec>
<colspec colnum="4" colname="4" colwidth="1.811in">
</colspec>
<thead>
<row rowsep="1"><html:tr>
<entry namest="1" nameend="2" align="center"><html:td valign="top" align="center" colspan="2" rowspan="1">
<p>Item
</p>
</html:td></entry>
<entry colname="3" morerows="1" align="center"><html:td valign="top" align="center" colspan="1" rowspan="2">
<p>FL display
</p>
</html:td></entry>
<entry colname="4" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>Key operation
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>Mode name
</p>
</html:td></entry>
<entry colname="2" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>Description
</p>
</html:td></entry>
<entry colname="4" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>Front Key
</p>
</html:td></entry>
</html:tr></row>
</thead>
<tbody>
<row rowsep="1"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>TEST Mode
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>&#42;All the main unit&#700;s parameters (include tuner) are initialized.
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<fig>
<graphic loc="graphic32" sizex="42.000mm" sizey="10.500mm"><html:img src="re080201.png" border="0"></html:img>
</graphic>
</fig>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Press [SKIP (REV)], [TIME SLIP] and [OPEN&#47;CLOSE] keys simultaneously for five seconds when power is off.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Service Mode
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Setting every kind of modes for servicing.
</p> 
<p>&#42;Details are described in &#8220; 
<emp>8. 3. Service Mode
</emp>&#8221;.
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<fig>
<graphic loc="graphic33" sizex="42.000mm" sizey="10.500mm"><html:img src="re080202.png" border="0"></html:img>
</graphic>
</fig>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>When the power is off, press [STOP], [TIME SLIP] and [OPEN&#47;CLOSE] keys simultaneously for 5 seconds.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Rating password
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>The audiovisual level setting password is initialized to &#8220;Level 8&#8221;.
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<fig>
<graphic loc="graphic34" sizex="42.000mm" sizey="10.500mm"><html:img src="re080203.png" border="0"></html:img>
</graphic>
</fig>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Open the tray, and press [SKIP (REV)] and [SKIP (FWD)] simultaneously for five seconds.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Forced disc eject
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Removing a disc that cannot be ejected.
</p> 
<p>The tray will open and unit will shift to P-off mode.
</p> 
<p>&#42;When Timer REC is ON or EXT-LINK is ON, execute " Forced disc eject " after releasing TimerREC
or EXT-LINK.</p> 
<p>&#42;This command is not effective during "Child lock" is ON.
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>The display before execution leaves.
</p> 
<fig>
<graphic loc="graphic35" sizex="42.000mm" sizey="10.500mm"><html:img src="re080204.png" border="0"></html:img>
</graphic>
</fig>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>When the power is off, press [STOP] and [CH UP] keys simultaneously for five seconds.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Child lock&#47;unlock
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Set or release &#8220;Child Lock&#8221;.
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<fig>
<graphic loc="graphic36" sizex="42.000mm" sizey="10.500mm"><html:img src="re080205.png" border="0"></html:img>
</graphic>
</fig>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Press [ENTER] and [RETURN] by remote controller simultaneously until [X-HOLD] is displayed.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>NTSC&#47;PAL system select
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>To switch PAL&#47; NTSC alternately.
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>The display before execution leaves.
</p> 
<fig>
<graphic loc="graphic37" sizex="42.000mm" sizey="10.500mm"><html:img src="re080206.png" border="0"></html:img>
</graphic>
</fig>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>When the power is on (E-E mode), press [STOP] and [OPEN&#47;CLOSE] simultaneously for five seconds.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Forced power-off
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>When the power button is not effective while power is ON, turn off the power forcibly.&#42;When Timer REC is ON or EXT-LINK is ON, execute &#8220;Forced Power-off&#8221; after releasing Timer RECor
EXT-LINK.</p> 
<p>Action:
</p> 
<p>The tray will open, and the power will turn off.
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Display in P-off mode.
</p>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Press [Power] key over than 10 seconds.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Aging
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Perform sequence of modes as &#42; Aging Description shown below continually.
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Display following the then mode.
</p>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>When the power is ON, press [CH DOWN], TIME SLIP] and [OPEN &#47; CLOSE] simultaneously for over five seconds and less than 10 seconds.
</p> 
<p>&#42;The [REC MODE] should be set to EP or LP.
</p> 
<p>&#42;Whenthe
unit has hung-up because of pressing keys for over 10 seconds, once turn off the power, and re-execute this command.</p> 
<p>&#8220;When releasing Aging mode, press [POWER] key.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" morerows="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="3">
<p>Demonstration lock&#47;unlock
</p>
</html:td></entry>
<entry colname="2" morerows="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="3">
<p>Ejection of the disc is prohibited.
</p> 
<p>The lock setting is effective until unlocking the tray and not released by &#8220;Main unit initialization&#8221; of service mode.
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>&#42;When lock the tray.
</p> 
<fig>
<graphic loc="graphic38" sizex="42.000mm" sizey="10.500mm"><html:img src="re080207.png" border="0"></html:img>
</graphic>
</fig> 
<p>&#8220;LOCK&#8221; is displayed for 3 seconds.
</p>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>When the power is on, press [STOP] and [POWER] keys simultaneously for five seconds.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>&#42;When unlock the tray.
</p> 
<fig>
<graphic loc="graphic39" sizex="42.000mm" sizey="10.500mm"><html:img src="re080208.png" border="0"></html:img>
</graphic>
</fig> 
<p>&#8220;UNLOCK&#8221; is displayed for 3 seconds.
</p>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>When the power is on, press [STOP] and [POWER] keys simultaneously for five seconds.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>&#42;When press OPEN&#47;CLOSE key while the tray being locked.
</p> 
<fig>
<graphic loc="graphic40" sizex="42.000mm" sizey="10.500mm"><html:img src="re080209.png" border="0"></html:img>
</graphic>
</fig> 
<p>Display &#8220;LOCK&#8221; for 3 seconds.
</p>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Press [OPEN&#47;CLOSE] key while the tray being locked.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>ATP re-execution
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Re-execute ATP.
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Display at ATP executing.
</p> 
<fig>
<graphic loc="graphic41" sizex="42.000mm" sizey="10.500mm"><html:img src="re080210.png" border="0"></html:img>
</graphic>
</fig>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>When the power is on (E-E mode), press [CH UP] and [CH DOWN] simultaneously for five seconds.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="0"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Progressive initialization
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>The progressive setting is initialized to Interlace.
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>The display before execution leaves.
</p> 
<fig>
<graphic loc="graphic42" sizex="42.000mm" sizey="10.500mm"><html:img src="re080211.png" border="0"></html:img>
</graphic>
</fig>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>When the power is on (E-E mode), press [STOP] and [TIME SLIP] simultaneously for five seconds.
</p>
</html:td></entry>
</html:tr></row>
</tbody>
</tgroup>
</html:table></table>
<topic>
<ttl>Aging Contents (Example):
</ttl>
<fig>
<graphic loc="graphic43" sizex="102.955mm" sizey="24.892mm"><html:img src="re080212.png" border="0"></html:img>
</graphic>
</fig>
</topic>
</ti2>
<ti2 column="3" newpage="1">
<ttl><html:a name="TITLE9_3">9.3 Service Modes </html:a>
</ttl>
<p>Service mode setting: While the power is off, press TIME SLIP, STOP and OPEN &#47; CLOSE simultaneously for five seconds.
</p>
<table frame="all" colsep="1" rowsep="1"><html:table frame="all" rules="all" >
<tgroup cols="4" colsep="1" rowsep="1">
<colspec colnum="1" colname="1" colwidth="1.299in">
</colspec>
<colspec colnum="2" colname="2" colwidth="2.283in">
</colspec>
<colspec colnum="3" colname="3" colwidth="1.811in">
</colspec>
<colspec colnum="4" colname="4" colwidth="1.811in">
</colspec>
<thead>
<row rowsep="1"><html:tr>
<entry namest="1" nameend="2" align="center"><html:td valign="top" align="center" colspan="2" rowspan="1">
<p>Item
</p>
</html:td></entry>
<entry colname="3" morerows="1" align="center"><html:td valign="top" align="center" colspan="1" rowspan="2">
<p>FL display
</p>
</html:td></entry>
<entry colname="4" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>Key operation
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>Mode name
</p>
</html:td></entry>
<entry colname="2" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>Description
</p>
</html:td></entry>
<entry colname="4" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>(Remote controller key)
</p>
</html:td></entry>
</html:tr></row>
</thead>
<tbody>
<row rowsep="1"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Release Items
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Item of Service Mode executing is cancelled.
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<fig>
<graphic loc="graphic44" sizex="40.000mm" sizey="10.500mm"><html:img src="re080301.png" border="0"></html:img>
</graphic>
</fig>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Press [0] [0] or [Return] in service mode.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Error Code Display
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Last Error Code of U14&#47;H&#47;F held by Timer is displayed on FL.
</p> 
<p>&#42;Details are described in 
<emp>&#8220;8. 1. Self-Diagnosis Functions&#8221;.
</emp>
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<fig>
<graphic loc="graphic45" sizex="40.000mm" sizey="20.000mm"><html:img src="re080302.png" border="0"></html:img>
</graphic>
</fig>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Press [0] [1] in service mode
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>ROM Version Display
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Region code, MAIN firm version, TIMER firm version and DRIVE firmware versions are displayed on FL for five seconds per each version in order, but ROM version will be left displayed.
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<fig>
<graphic loc="graphic46" sizex="40.000mm" sizey="62.000mm"><html:img src="re080303.png" border="0"></html:img>
</graphic>
</fig> 
<p> &#8220; 
<graphic loc="graphic47" sizex="2.700mm" sizey="4.800mm"><html:img src="kome.png" border="0"></html:img>
</graphic>&#8221;are version displays.
</p>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Press [0] [2] in service mode
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry namest="1" nameend="4" align="justify"><html:td valign="top" align="justify" colspan="4" rowspan="1">
<fig>
<graphic loc="graphic48" sizex="182.000mm" sizey="136.991mm"><html:img src="re080304.png" border="0"></html:img>
</graphic>
</fig>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" morerows="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="2">
<p>White Picture Output
</p>
</html:td></entry>
<entry colname="2" morerows="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="2">
<p>White picture is output as component Output from AV Decoder.
</p> 
<p>&#42;White picture
</p> 
<p>(Saturation rate : 100&#37;)
</p> 
<p>&#42;It is enable to switch Interlace&#47;Progressive by &#8220;I&#47;P switch:
[1] [4]&#8221; </p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>&#42;Initial mode is &#8220;Interlace&#8221;.
</p> 
<fig>
<graphic loc="graphic49" sizex="40.000mm" sizey="10.500mm"><html:img src="re080305.png" border="0"></html:img>
</graphic>
</fig>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Press [1] [1] in service mode.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Switch Interlace&#47;Progressive
</p> 
<fig>
<graphic loc="graphic50" sizex="40.000mm" sizey="10.500mm"><html:img src="re080306.png" border="0"></html:img>
</graphic>
</fig>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Press [1] [4] in White Picture Output mode.
</p> 
<p>&#42;I&#47;P are switched alternately.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" morerows="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="2">
<p>Magenta Picture Output
</p>
</html:td></entry>
<entry colname="2" morerows="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="2">
<p>Magenta picture is output with Component Output from AV Decoder.
</p> 
<p>&#42;Magenta picture
</p> 
<p>(Saturation rate: 100&#37;)
</p> 
<p>&#42;It is enable to switch Interlace&#47;Progressive by &#8220;I&#47;P switch:
[1] [4]&#8221; </p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>&#42;Initial mode is &#8220;Interlace&#8221;.
</p> 
<fig>
<graphic loc="graphic51" sizex="40.000mm" sizey="10.500mm"><html:img src="re080307.png" border="0"></html:img>
</graphic>
</fig>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Press [1] [2] in service mode.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Switch Interlace&#47;Progressive
</p> 
<fig>
<graphic loc="graphic52" sizex="40.000mm" sizey="10.500mm"><html:img src="re080308.png" border="0"></html:img>
</graphic>
</fig>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Press [1] [4] in Magenta Picture Output mode.
</p> 
<p>&#42;I&#47;P are switched alternately.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" morerows="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="3">
<p>RTSC Return in XP
</p> 
<p>(A &#38; V)
</p>
</html:td></entry>
<entry colname="2" morerows="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="3">
<p>AV1 input signal is encoded (XP), decoded (XP) and output decoded signal to external without DISC recording and DISC playback.
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Initial mode: EE2&#47; Interlace&#47; XP&#47; Audio 48kHz
</p> 
<fig>
<graphic loc="graphic53" sizex="40.000mm" sizey="10.500mm"><html:img src="re080309.png" border="0"></html:img>
</graphic>
</fig>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Press [1] [3] in service mode.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Switch Interlace&#47;Progressive
</p> 
<fig>
<graphic loc="graphic54" sizex="40.000mm" sizey="10.500mm"><html:img src="re080310.png" border="0"></html:img>
</graphic>
</fig>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Press [1] [4] in RTSC Return XP mode.
</p> 
<p>&#42;I&#47;P are switched alternately.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Audio 44.1 kHz&#47; 48 kHz Switch
</p> 
<fig>
<graphic loc="graphic55" sizex="40.000mm" sizey="10.500mm"><html:img src="re080311.png" border="0"></html:img>
</graphic>
</fig>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Press [2] [4] in RTSC Return XP mode.
</p> 
<p>&#42;48 kHz &#47; 44.1 kHz are switched alternately.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>I&#47;P Switch
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Switch Interlace and Progressive in EE mode.
</p> 
<p>&#42;Initial setting is &#8220;Interlace&#8221;.
</p> 
<p>&#42;This command is effective during executing &#8220;White Picture Output&#8221;, &#8220;Magenta Picture
Output&#8221; and &#8220;RTSC Return in XP (A &#38; V)&#8221; modes.</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Initial mode is Interlace
</p> 
<fig>
<graphic loc="graphic56" sizex="40.000mm" sizey="10.500mm"><html:img src="re080312.png" border="0"></html:img>
</graphic>
</fig> 
<p>Switch Interlace&#47;Progressive
</p> 
<fig>
<graphic loc="graphic57" sizex="40.000mm" sizey="10.500mm"><html:img src="re080313.png" border="0"></html:img>
</graphic>
</fig>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Press [1] [4] in I&#47;P Switch mode.
</p> 
<p>&#42;I&#47;P are switched alternately.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Audio Mute (XTMUTE)
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Check whether mute is applied normally by the timer microprocessor.
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<fig>
<graphic loc="graphic58" sizex="40.000mm" sizey="10.500mm"><html:img src="re080314.png" border="0"></html:img>
</graphic>
</fig>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Press [2] [1] in service mode.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Audio Mute (XDMUTE)
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Check whether mute is applied normally by the Digital P.C.B. (GLUE IC).
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<fig>
<graphic loc="graphic59" sizex="40.000mm" sizey="10.500mm"><html:img src="re080315.png" border="0"></html:img>
</graphic>
</fig>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Press [2] [2] in service mode.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" morerows="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="2">
<p>Audio Pattern Output
</p>
</html:td></entry>
<entry colname="2" morerows="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="2">
<p>The audio pattern stored in the internal memory is output
</p> 
<p>(Lch: 1kHz&#47;-18dB)
</p> 
<p>(Rch: 400Hz&#47;-18dB)
</p> 
<p>&#42;Audio sound clock switching operation of DAC can
be confirmed by sub command [2] [4].</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Initial mode (Audio 48kHz)
</p> 
<fig>
<graphic loc="graphic60" sizex="40.000mm" sizey="10.500mm"><html:img src="re080316.png" border="0"></html:img>
</graphic>
</fig>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Press [2] [3] in service mode.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Audio 44.1kHz&#47;48kHz switching
</p> 
<fig>
<graphic loc="graphic61" sizex="40.000mm" sizey="10.500mm"><html:img src="re080317.png" border="0"></html:img>
</graphic>
</fig>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Press [2] [4] in Audio Pattern Output mode.
</p> 
<p>&#42;48 kHz &#47; 44.1 kHz are switched alternately.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>HDD READ inspection
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Perform a complete read inspection of the HDD.
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>When the HDD is OK
</p> 
<fig>
<graphic loc="graphic62" sizex="40.000mm" sizey="10.500mm"><html:img src="re0803a.png" border="0"></html:img>
</graphic>
</fig> 
<p>If the HDD is defective
</p> 
<fig>
<graphic loc="graphic63" sizex="40.000mm" sizey="68.000mm"><html:img src="re0803b.png" border="0"></html:img>
</graphic>
</fig>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Press [3] [1] in the service mode.
</p> 
<p>&#42;When canceling the checking mode while executing, do "forced power-off".
</p> 
<p>Method:
</p> 
<p>Press the "POWER" button on the Front Panel more than 10 seconds.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Laser Used Time Indication
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Check laser used time (hours) of drive.
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<fig>
<graphic loc="graphic64" sizex="40.000mm" sizey="10.500mm"><html:img src="re080318.png" border="0"></html:img>
</graphic>
</fig> 
<p>&#8226;(&#42;&#42;&#42;&#42;&#42;) is the used time display in hour.
</p> 
<p>&#8226;Laser used time
of DVD&#47; CD in Playback&#47;Recording mode is counted.</p>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Press [4] [1] in service mode.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Delete the Laser Used Time
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Laser used time stored in the memory of the unit is deleted.
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<fig>
<graphic loc="graphic65" sizex="42.000mm" sizey="10.500mm"><html:img src="re080319.png" border="0"></html:img>
</graphic>
</fig>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Press [9] [5] in service mode.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>RAM Drive Last Error
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>RAM Drive error code display.
</p> 
<p>&#42;For details about the drive error code, refer to the Service Manual for the specific RAM Drive.
</p> 
<p>&#42;Details are described in &#8220; 
<emp>7. Service Explorer
</emp>&#8221;.
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>1. Error Number is displayed for 5 seconds.
</p> 
<fig>
<graphic loc="graphic66" sizex="40.000mm" sizey="10.500mm"><html:img src="re080320.png" border="0"></html:img>
</graphic>
</fig> 
<p>2. Time when the error has occurred is displayed for 5 seconds.
</p> 
<fig>
<graphic loc="graphic67" sizex="40.000mm" sizey="10.500mm"><html:img src="re080321.png" border="0"></html:img>
</graphic>
</fig> 
<p>Y: Year
</p> 
<p>MM: Month
</p> 
<p>DD: Day
</p> 
<p>hh: Hour
</p> 
<p>mm: Minute
</p> 
<p>ss: Second
</p> 
<p>3. Last Drive Error (1&#47;2) is displayed for 5 seconds.
</p> 
<fig>
<graphic loc="graphic68" sizex="40.000mm" sizey="10.500mm"><html:img src="re080322.png" border="0"></html:img>
</graphic>
</fig> 
<p>4. Last Drive Error (2&#47;2) is displayed for 5 seconds.
</p> 
<fig>
<graphic loc="graphic69" sizex="40.000mm" sizey="10.500mm"><html:img src="re080323.png" border="0"></html:img>
</graphic>
</fig> 
<p>5. Error occurring Disc type is
displayed for 5 seconds.</p> 
<fig>
<graphic loc="graphic70" sizex="40.000mm" sizey="10.500mm"><html:img src="re080324.png" border="0"></html:img>
</graphic>
</fig> 
<p>6. Disc Maker ID is displayed for 5 seconds.
</p> 
<fig>
<graphic loc="graphic71" sizex="40.000mm" sizey="10.500mm"><html:img src="re080325.png" border="0"></html:img>
</graphic>
</fig> 
<p>7. Factor of
Drive Erroroccurring is left displayed</p> 
<fig>
<graphic loc="graphic72" sizex="40.000mm" sizey="10.500mm"><html:img src="re080326.png" border="0"></html:img>
</graphic>
</fig>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Press [4] [2] in service mode.
</p> 
<p>Then press [0] [1] ~ [9] [9], the past 99 errors are displayed.
</p> 
<p>
</p> 
<p>
</p> 
<p>
</p> 
<p>
</p> 
<p>
</p> 
<p>
</p> 
<p>
</p> 
<p>
</p> 
<p>
</p> 
<p>
</p> 
<p>
</p> 
<p>
</p> 
<p>
</p> 
<p>
</p> 
<p>
</p> 
<p>
</p> 
<p>
</p> 
<p>
</p> 
<p>
</p> 
<p>
</p> 
<p>
</p> 
<p>
</p> 
<p>
</p> 
<p>
</p> 
<p>
</p> 
<p>
</p> 
<p>
</p> 
<p>
</p> 
<p>
</p> 
<p>
</p> 
<p>
</p> 
<p>
</p> 
<p>
</p> 
<p>Incase
that the supplier cannot be identified, display is black out.</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Delete the Last Drive Error
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Delete the Last Drive Error information stored on the DVD RAM-Drive.
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<fig>
<graphic loc="graphic73" sizex="40.000mm" sizey="10.500mm"><html:img src="re080327.png" border="0"></html:img>
</graphic>
</fig>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Press [9] [6] in service mode.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Turn on all FL&#47;LEDs
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>All segments of FL and all LEDs are turned on.
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>All segments are turned on.
</p>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Press [5] [1] in service mode.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>PB HIGH Signal Output
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>8 pin of AV 1 Jack (PB HIGH terminal) is High (approx. 11V DC).
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<fig>
<graphic loc="graphic74" sizex="40.000mm" sizey="10.500mm"><html:img src="re080328.png" border="0"></html:img>
</graphic>
</fig>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Press [5] [2] in service mode.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>PB MIDDLE Signal Output
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>8 pin of AV 1 Jack (PB HIGH terminal) is Middle (approx. 5.5V DC).
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<fig>
<graphic loc="graphic75" sizex="40.000mm" sizey="10.500mm"><html:img src="re080329.png" border="0"></html:img>
</graphic>
</fig>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Press [5] [3] in service mode.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Front connection inspection
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Press all front keys and check the connection between Main P.C.B. and Front P.C.B.
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<fig>
<graphic loc="graphic76" sizex="40.000mm" sizey="16.000mm"><html:img src="re080330.png" border="0"></html:img>
</graphic>
</fig> 
<p>(1) Each time a key is pressed, segment turned on increases one by one.
</p> 
<p>(2) Total umber of keys that have been pressed.
</p>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Press [5] [4] in service mode.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Production Date Display
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Display the date when the unit was produced.
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<fig>
<graphic loc="graphic77" sizex="40.000mm" sizey="10.500mm"><html:img src="re080331.png" border="0"></html:img>
</graphic>
</fig> 
<p>YYY: Year
</p> 
<p>MM: Month
</p> 
<p>DD: Day
</p>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Press [6] [1] in service mode.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Display the accumulated working time
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Display the accumulated unit&#8217;s working time.
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<fig>
<graphic loc="graphic78" sizex="40.000mm" sizey="10.500mm"><html:img src="re080332.png" border="0"></html:img>
</graphic>
</fig> 
<p>(Indicating unit: Second)
</p>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Press [6] [4] in service mode.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Display the Error History
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Display the Error History stored on the unit.
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Display reason of error for 5 seconds.
</p> 
<fig>
<graphic loc="graphic79" sizex="42.000mm" sizey="10.500mm"><html:img src="re080333.png" border="0"></html:img>
</graphic>
</fig> 
<p>Display the time when the error has occurred for 5 seconds.
</p> 
<fig>
<graphic loc="graphic80" sizex="42.000mm" sizey="10.500mm"><html:img src="re080334.png" border="0"></html:img>
</graphic>
</fig> 
<p>YY: Year
</p> 
<p>MM: Month
</p> 
<p>DD: Day
</p> 
<p>HH: Hour
</p> 
<p>MM: Minute
</p> 
<p>Display the accumulated working time to occurring of the error for 5 seconds.
</p> 
<fig>
<graphic loc="graphic81" sizex="42.000mm" sizey="10.500mm"><html:img src="re080335.png" border="0"></html:img>
</graphic>
</fig> 
<p>(Indicating unit: Second)
</p>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Press [6] [5] in service mode.
</p> 
<p>Then press [0] [1] ~ [1] [9], the past 19 error histories are displayed.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Delete the Error History
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Delete Error History information stored on the unit.
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<fig>
<graphic loc="graphic82" sizex="42.000mm" sizey="10.500mm"><html:img src="re080336.png" border="0"></html:img>
</graphic>
</fig>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Press [9] [7] in service mode.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>AV4(V)&#47;AV1(RGB) I&#47;O Setting
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Set input to AV4(V) and set output to AV1(RGB) for I&#47;O checking
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<fig>
<graphic loc="graphic83" sizex="42.000mm" sizey="10.500mm"><html:img src="re080337.png" border="0"></html:img>
</graphic>
</fig>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Press [8] [0] in service mode.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>AV2(Y&#47;C)&#47;AV1(V) I&#47;O Setting
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Set input to AV2(Y&#47;C) and set output to AV1(V) for I&#47;O checking
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<fig>
<graphic loc="graphic84" sizex="42.000mm" sizey="10.500mm"><html:img src="re080338.png" border="0"></html:img>
</graphic>
</fig>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Press [8] [1] in service mode.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>AV2(V)&#47;AV1(Y&#47;C) I&#47;O Setting
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Set input to AV2(V) and set output to AV1(Y&#47;C) for I&#47;O checking
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<fig>
<graphic loc="graphic85" sizex="42.000mm" sizey="10.500mm"><html:img src="re080339.png" border="0"></html:img>
</graphic>
</fig>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Press [8] [2] in service mode.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>AV2(RGB)&#47;AV1(V) I&#47;O Setting
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Set input to AV2(RGB) and set output to AV1(V) for I&#47;O checking
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<fig>
<graphic loc="graphic86" sizex="42.000mm" sizey="10.500mm"><html:img src="re080340.png" border="0"></html:img>
</graphic>
</fig>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Press [8] [3] in service mode.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>P50 (H) Output
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Timer Microprocessor IC7501-22 output High signal for AV1-pin 10 passing through inverter (approx. 0V DC at AV1-pin 10).
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<fig>
<graphic loc="graphic87" sizex="42.000mm" sizey="10.500mm"><html:img src="re080341.png" border="0"></html:img>
</graphic>
</fig> 
<p>When OK.
</p> 
<fig>
<graphic loc="graphic88" sizex="42.000mm" sizey="10.500mm"><html:img src="re080342.png" border="0"></html:img>
</graphic>
</fig> 
<p>When NG.
</p> 
<fig>
<graphic loc="graphic89" sizex="42.000mm" sizey="10.500mm"><html:img src="re080343.png" border="0"></html:img>
</graphic>
</fig>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Press [8] [4] in service mode.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>P50 (L) Output
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Timer Microprocessor IC7501-22 output Low signal for AV1-pin 10 passing through inverter (approx. 4.4 V DC at AV1-pin 10).
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<fig>
<graphic loc="graphic90" sizex="42.000mm" sizey="10.500mm"><html:img src="re080344.png" border="0"></html:img>
</graphic>
</fig> 
<p>When OK.
</p> 
<fig>
<graphic loc="graphic91" sizex="42.000mm" sizey="10.500mm"><html:img src="re080345.png" border="0"></html:img>
</graphic>
</fig> 
<p>When NG.
</p> 
<fig>
<graphic loc="graphic92" sizex="42.000mm" sizey="10.500mm"><html:img src="re080346.png" border="0"></html:img>
</graphic>
</fig>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Press [8] [5] in service mode.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Tray OPEN&#47;CLOSE Test
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>The RAM drive tray is opened and closed repeatedly.
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<fig>
<graphic loc="graphic93" sizex="42.000mm" sizey="10.500mm"><html:img src="re080347.png" border="0"></html:img>
</graphic>
</fig> 
<p>&#8220;&#42;&#8221; is number of open&#47;close cycle times.
</p>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Press [9] [1] in service mode
</p> 
<p>&#42;When releasing this mode, press the [POWER] button on Front Panel more than 10 seconds.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Error code initialization
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Initialization of the last error code held by timer (Write in F00)
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<fig>
<graphic loc="graphic94" sizex="42.000mm" sizey="10.500mm"><html:img src="re080348.png" border="0"></html:img>
</graphic>
</fig>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Press [9] [8] in service mode.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="1"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Initialize Service
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Last Drive Error, Error history and Error Codes stored on the unit are initialized to factory setting.
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<fig>
<graphic loc="graphic95" sizex="42.000mm" sizey="10.500mm"><html:img src="re080349.png" border="0"></html:img>
</graphic>
</fig>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Press [9] [9] in service mode.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="0"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Finishing service mode
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Release Service Mode.
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Display in STOP (E-E) mode.
</p> 
<fig>
<graphic loc="graphic96" sizex="42.000mm" sizey="10.500mm"><html:img src="re080350.png" border="0"></html:img>
</graphic>
</fig>
</html:td></entry>
<entry colname="4" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>Press power button on the front panel in service mode.
</p>
</html:td></entry>
</html:tr></row>
</tbody>
</tgroup>
</html:table></table>
</ti2>
</other>
</html:body>
</svctechdoc>
