<?xml version="1.0" encoding="utf-8"?>
<?xml-stylesheet href="DSD0405014C8.css" type="text/css"?>
<!-- DC Version =\\\\\\\\ "(unknown).0.0.1" -->
<!-- Character entity set. Typical invocation:
     <!ENTITY % ISOnum PUBLIC
       "ISO 8879-1986//ENTITIES Numeric and Special Graphic//EN">
     %ISOnum;
-->
<svctechdoc lang="english" type="svc" xmlns:html="http://www.w3.org/Profiles/XHTML-transitional">
<html:script language="JavaScript" src="script.js"></html:script>
<html:script language="JavaScript" src="tree.js"></html:script>
<html:body onload="dgfFsetClose();setScroll();">
<other>
<ttl><html:a name="TITLE13">13 Adjustment Procedures </html:a>
</ttl>
<ti2 column="3">
<ttl><html:a name="TITLE13_1">13.1 After replacing the RAM Drive with new one </html:a>
</ttl>
<fig>
<graphic loc="graphic127" sizex="183.000mm" sizey="10.075mm"><html:img src="re120101.png" border="0"></html:img>
</graphic>
</fig>
</ti2>
<ti2 column="3">
<ttl><html:a name="TITLE13_2">13.2 When the unit does not operate normally after replacing the Timer Microprocessor with new one </html:a>
</ttl>
<p>in order to transmit the
</p>
<table frame="all" colsep="1" rowsep="1"><html:table frame="all" rules="all" >
<tgroup cols="3" colsep="1" rowsep="1">
<colspec colnum="1" colname="1" colwidth="0.787in">
</colspec>
<colspec colnum="2" colname="2" colwidth="3.543in">
</colspec>
<colspec colnum="3" colname="3" colwidth="2.874in">
</colspec>
<thead>
<row rowsep="1"><html:tr>
<entry colname="1" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>
<emp>Step
</emp>
</p>
</html:td></entry>
<entry colname="2" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>
<emp>Operation
</emp>
</p>
</html:td></entry>
<entry colname="3" align="center"><html:td valign="top" align="center" colspan="1" rowspan="1">
<p>
<emp>Descriptions
</emp>
</p>
</html:td></entry>
</html:tr></row>
</thead>
<tbody>
<row rowsep="0"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>1
</p>
</html:td></entry>
<entry colname="2" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>While power is ON, short IC7508-4 pin (RESET) and the GND.
</p>
</html:td></entry>
<entry colname="3" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>&#8220;RESET (L)&#8221; is transmitted to the reset terminal of Timer Microprocessor (IC7501-11 pin), then the unit operates normally.
</p>
</html:td></entry>
</html:tr></row>
</tbody>
</tgroup>
</html:table></table>
</ti2>
</other>
</html:body>
</svctechdoc>
