<?xml version="1.0" encoding="utf-8"?>
<?xml-stylesheet href="DSD0405014C8.css" type="text/css"?>
<!-- DC Version =\\\\\\\\ "(unknown).0.0.1" -->
<!-- Character entity set. Typical invocation:
     <!ENTITY % ISOnum PUBLIC
       "ISO 8879-1986//ENTITIES Numeric and Special Graphic//EN">
     %ISOnum;
-->
<svctechdoc lang="english" type="svc" xmlns:html="http://www.w3.org/Profiles/XHTML-transitional">
<html:script language="JavaScript" src="script.js"></html:script>
<html:script language="JavaScript" src="tree.js"></html:script>
<html:body onload="dgfFsetClose();setScroll();">
<other>
<ttl><html:a name="TITLE10">10 Assembling and Disassembling </html:a>
</ttl>
<ti2 column="3">
<ttl><html:a name="TITLE10_1">10.1 Disassembly Flow Chart </html:a>
</ttl>
<p>The following chart is the procedure for disassembling the casing and inside parts for internal inspection when carrying out the servicing.
</p>
<p>To assemble the unit, reverse the steps shown in the chart below.
</p>
<fig>
<graphic loc="graphic97" sizex="176.530mm" sizey="61.468mm"><html:img src="re_da_01.png" border="0"></html:img>
</graphic>
</fig>
</ti2>
<ti2 column="3">
<ttl><html:a name="TITLE10_2">10.2 P.C.B. Positions </html:a>
</ttl>
<fig>
<graphic loc="graphic98" sizex="163.830mm" sizey="126.831mm"><html:img src="re_da_02.png" border="0"></html:img>
</graphic>
</fig>
</ti2>
<ti2 newpage="1">
<ttl><html:a name="TITLE10_3">10.3 Top Case </html:a>
</ttl>
<ol>
<li>
<p>Remove the 2 screws (A) and 3 screws (B).
</p>
</li>
<li>
<p>Open the both ends at rear side of the Top Case a little and lift the Top Case in the direction of the arrows.
</p>
</li>
</ol>
<fig>
<graphic loc="graphic99" sizex="88.500mm" sizey="99.310mm"><html:img src="re_da_03.png" border="0"></html:img>
</graphic>
</fig>
</ti2>
<ti2>
<ttl><html:a name="TITLE10_4">10.4 Digital P.C.B. </html:a>
</ttl>
<fig>
<graphic loc="graphic100" sizex="88.500mm" sizey="35.821mm"><html:img src="re1004a.png" border="0"></html:img>
</graphic>
</fig>
<ol>
<li>
<p>Remove the FFC and a Screw.
</p>
</li>
<li>
<p>Unlock a Rocking Spacer.
</p>
</li>
<li>
<p>Lift up Digital P.C.B. slightly so to disconnect Connector to remove Digital P.C.B.
</p>
<fig>
<graphic loc="graphic101" sizex="88.500mm" sizey="71.099mm"><html:img src="re_da_04.png" border="0"></html:img>
</graphic>
</fig>
</li>
</ol>
<caution>
<ttl>CAUTION:
</ttl>
<p>When replacing Digital P.C.B., pay attention as below.
</p>
</caution>
<fig>
<graphic loc="graphic102" sizex="88.500mm" sizey="164.785mm"><html:img src="re_da_05.png" border="0"></html:img>
</graphic>
</fig>
</ti2>
<ti2 newpage="1">
<ttl><html:a name="TITLE10_5">10.5 Front Panel </html:a>
</ttl>
<ol>
<li>
<p>Remove 3 tabs (A) and 2 tabs (B) in this order. (The tab (A) and (B) should be removed at the same time, respectively.)
</p>
<fig>
<graphic loc="graphic103" sizex="88.500mm" sizey="58.531mm"><html:img src="re_da_06.png" border="0"></html:img>
</graphic>
</fig>
</li>
<li>
<p>Move the front panel to front side straight and slowly so to remove it with Connector.
</p>
<fig>
<graphic loc="graphic104" sizex="88.500mm" sizey="59.586mm"><html:img src="re_da_07.png" border="0"></html:img>
</graphic>
</fig>
</li>
</ol>
</ti2>
<ti2>
<ttl><html:a name="TITLE10_6">10.6 Front (R) P.C.B. </html:a>
</ttl>
<ol>
<li>
<p>Remove 6 screws and Front Angle.
</p>
<fig>
<graphic loc="graphic105" sizex="88.500mm" sizey="49.743mm"><html:img src="re_da_08.png" border="0"></html:img>
</graphic>
</fig>
</li>
</ol>
</ti2>
<ti2 newcol="1">
<ttl><html:a name="TITLE10_7">10.7 HDD </html:a>
</ttl>
<fig>
<graphic loc="graphic106" sizex="88.500mm" sizey="36.580mm"><html:img src="re0907a.png" border="0"></html:img>
</graphic>
</fig>
<ol>
<li>
<p>Remove 3 Screws (A) and 2 connectors.
</p>
</li>
<li>
<p>Slide and lift up HDD Holder in the direction of the arrows so to unlock 3 locking tabs.
</p>
<fig>
<graphic loc="graphic107" sizex="88.500mm" sizey="71.099mm"><html:img src="re_da_09.png" border="0"></html:img>
</graphic>
</fig>
<fig>
<graphic loc="graphic108" sizex="88.500mm" sizey="62.135mm"><html:img src="re_da_10.png" border="0"></html:img>
</graphic>
</fig>
<topic newpage="1">
<ttl>
</ttl>
</topic>
</li>
<li>
<p>Lift up HDD with super sheet vertically and remove super sheet.
</p>
<fig>
<graphic loc="graphic109" sizex="88.500mm" sizey="75.933mm"><html:img src="re_da_11.png" border="0"></html:img>
</graphic>
</fig>
<table frame="all" colsep="0" rowsep="0"><html:table frame="all" rules="all" >
<tgroup cols="1" colsep="0" rowsep="0">
<colspec colnum="1" colname="1" colwidth="3.484in" colsep="0">
</colspec>
<tbody>
<row rowsep="0"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>
<emp>Handling of HDD
</emp>
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="0"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<p>The following precautions should be taken when handling HDD.
</p>
</html:td></entry>
</html:tr></row>
<row rowsep="0"><html:tr>
<entry colname="1" align="justify"><html:td valign="top" align="justify" colspan="1" rowspan="1">
<ol>
<li>
<p>Never give an impact to HDD. (Even a drop from 1cm height can be a cause of HDD failure.
</p>
</li>
<li>
<p>When placing HDD on a workbench, provide a mat on a bench for shock absorption and anti-static purposes.
</p>
</li>
<li>
<p>When installing HDD, release it from your hands only after confirming that it is fully set on the chassis.
</p>
</li>
<li>
<p>Avoid stacking up HDD.
</p>
</li>
<li>
<p>HDD is unstable and easy to fall. Do not stand it on its side face.
</p>
</li>
<li>
<p>When handling HDD, hold its side faces to avoid static hazard.
</p>
</li>
<li>
<p>Do not place HDD on its wrapping bag after removal. (Prevention of static hazard
</p>
</li>
<li>
<p>Use a screwdriver with low impact and anti-static features.
</p>
</li>
<li>
<p>To replace HDD, remove the vertical short-circuit pin.
</p>
<p>(Keep the horizontal short-circuit pin in its place)
</p>
</li>
</ol>
</html:td></entry>
</html:tr></row>
<row rowsep="0"><html:tr>
<entry colname="1" align="left"><html:td valign="top" align="left" colspan="1" rowspan="1">
<topic>
<ttl>Note:
</ttl>
<p>When replacing HDD, please make the rear jumper slave or cable select configuration.
</p>
<p>(same configuration as HDD to exchange)
</p>
</topic>
</html:td></entry>
</html:tr></row>
</tbody>
</tgroup>
</html:table></table>
</li>
</ol>
</ti2>
<ti2 newcol="1">
<ttl><html:a name="TITLE10_8">10.8 HDD Bracket </html:a>
</ttl>
<ol>
<li>
<p>Remove 4 screws (B) and HDD Bracket with 2 Insulation Sheets.
</p>
<fig>
<graphic loc="graphic110" sizex="88.500mm" sizey="71.099mm"><html:img src="re_da_12.png" border="0"></html:img>
</graphic>
</fig>
</li>
</ol>
</ti2>
<ti2>
<ttl><html:a name="TITLE10_9">10.9 DVD-RAM Drive </html:a>
</ttl>
<ol>
<li>
<p>Remove 3 Screws.
</p>
</li>
<li>
<p>Pull out DVD-RAM Drive vertically so to remove it with Connector.
</p>
<fig>
<graphic loc="graphic111" sizex="88.500mm" sizey="76.372mm"><html:img src="re_da_13.png" border="0"></html:img>
</graphic>
</fig>
</li>
</ol>
</ti2>
<ti2 newpage="1">
<ttl><html:a name="TITLE10_10">10.10 Rear Panel </html:a>
</ttl>
<ol>
<li>
<p>Remove the 12 screws (A) and screw (B).
</p>
</li>
<li>
<p>Unlock 2 Locking Tabs to remove Rear Panel.
</p>
<fig>
<graphic loc="graphic112" sizex="88.500mm" sizey="64.332mm"><html:img src="re_da_14.png" border="0"></html:img>
</graphic>
</fig>
</li>
</ol>
<ti3 module="0">
<ttl><html:a name="TITLE10_10_1">10.10.1 Only Fan Motor </html:a>
</ttl>
<ol>
<li>
<p>Remove the 2 screws.
</p>
<fig>
<graphic loc="graphic113" sizex="88.500mm" sizey="51.676mm"><html:img src="re_da_15.png" border="0"></html:img>
</graphic>
</fig>
</li>
<li>
<p>Remove Fan Connector to remove Fan Motor.
</p>
<fig>
<graphic loc="graphic114" sizex="88.500mm" sizey="82.700mm"><html:img src="re_da_16.png" border="0"></html:img>
</graphic>
</fig>
</li>
</ol>
</ti3>
</ti2>
<ti2 newcol="1">
<ttl><html:a name="TITLE10_11">10.11 Main P.C.B. </html:a>
</ttl>
<ol>
<li>
<p>Remove the 7 screws (A), Connector (A) and Fan Connector.
</p>
<fig>
<graphic loc="graphic115" sizex="88.500mm" sizey="91.928mm"><html:img src="re_da_17.png" border="0"></html:img>
</graphic>
</fig>
</li>
<li>
<p>Remove a Screw (B) and lift up Front Jack portion of Main P.C.B. slightly so to unlock Tab to remove Main P.C.B..
</p>
<fig>
<graphic loc="graphic116" sizex="88.500mm" sizey="55.543mm"><html:img src="re_da_18.png" border="0"></html:img>
</graphic>
</fig>
</li>
</ol>
</ti2>
<ti2 newpage="1">
<ttl><html:a name="TITLE10_12">10.12 Power P.C.B. </html:a>
</ttl>
<ol>
<li>
<p>Lift up Power P.C.B. a little so to unlock 2 Tabs and slide Power P.C.B. so to unlock Flange to remove Power P.C.B.
</p>
<fig>
<graphic loc="graphic117" sizex="88.500mm" sizey="87.709mm"><html:img src="re_da_19.png" border="0"></html:img>
</graphic>
</fig>
</li>
</ol>
</ti2>
<ti2>
<ttl><html:a name="TITLE10_13">10.13 The Scart P.C.B. </html:a>
</ttl>
<ol>
<li>
<p>Pull out the Scart P.C.B. in the direction of the arrow.
</p>
<fig>
<graphic loc="graphic118" sizex="88.500mm" sizey="61.053mm"><html:img src="re_da_20.png" border="0"></html:img>
</graphic>
</fig>
</li>
</ol>
<topic>
<ttl>Note:
</ttl>
<p>At first disconnect the connector on one side, and pull out the Scart P.C.B.
</p>
<fig>
<graphic loc="graphic119" sizex="53.340mm" sizey="28.448mm"><html:img src="re_da_21.png" border="0"></html:img>
</graphic>
</fig>
</topic>
</ti2>
<ti2 newcol="1">
<ttl><html:a name="TITLE10_14">10.14 VIF Decoder P.C.B. and Nicam Decoder P.C.B. </html:a>
</ttl>
<ol>
<li>
<p>Remove the solders.
</p>
</li>
<li>
<p>Pull out the VIF Decoder P.C.B. and Nicam Decoder P.C.B.
</p>
<fig>
<graphic loc="graphic120" sizex="88.500mm" sizey="107.766mm"><html:img src="re_da_22.png" border="0"></html:img>
</graphic>
</fig>
</li>
</ol>
</ti2>
</other>
</html:body>
</svctechdoc>
