<?xml version="1.0" encoding="utf-8"?>
<?xml-stylesheet href="DSD0405014C8.css" type="text/css"?>
<!-- DC Version =\\\\\\\\ "(unknown).0.0.1" -->
<!-- Character entity set. Typical invocation:
     <!ENTITY % ISOnum PUBLIC
       "ISO 8879-1986//ENTITIES Numeric and Special Graphic//EN">
     %ISOnum;
-->
<svctechdoc lang="english" type="svc" xmlns:html="http://www.w3.org/Profiles/XHTML-transitional">
<html:script language="JavaScript" src="script.js"></html:script>
<html:script language="JavaScript" src="tree.js"></html:script>
<html:body onload="dgfFsetClose();setScroll();">
<other>
<ttl><html:a name="TITLE2">2 Safety precautions </html:a>
</ttl>
<ti2 column="2">
<ttl><html:a name="TITLE2_1">2.1 General guidelines </html:a>
</ttl>
<ol column="2">
<li>
<p>When servicing, observe the original lead dress. If a short circuit is found, replace all parts which have been overheated or damaged by the short circuit.
</p>
</li>
<li>
<p>After servicing, see to it that all the protective devices such as insulation barriers, insulation papers shields are properly installed.
</p>
</li>
<li>
<p>After servicing, make the following leakage current checks to prevent the customer from being exposed to shock hazards.
</p>
</li>
</ol>
<ti3>
<ttl><html:a name="TITLE2_1_1">2.1.1 Leakage current cold check </html:a>
</ttl>
<ol>
<li>
<p>Unplug the AC cord and connect a jumper between the two prongs on the plug.
</p>
</li>
<li>
<p>Measure the resistance value, with an ohmmeter, between the jumpered AC plug and each exposed metallic cabinet part on the equipment such as screwheads, connectors, control shafts, etc. When the exposed metallic part has a return path to thechassis,
the reading should be between 1M&#8486; and 5.2M&#8486;.<br><html:br></html:br>
</br> When the exposed metal does not have a return path to the chassis, the reading must be 
<graphic loc="graphic3" sizex="3.566mm" sizey="4.686mm"><html:img src="mugen.png" border="0"></html:img>
</graphic>.
</p>
<fig>
<cap id="behggcij">Figure 1
</cap>
<graphic loc="graphic4" sizex="88.500mm" sizey="40.138mm"><html:img src="re010101.png" border="0"></html:img>
</graphic>
</fig>
</li>
</ol>
</ti3>
<ti3 newcol="1">
<ttl><html:a name="TITLE2_1_2">2.1.2 Leakage current hot check </html:a>
<br><html:br></html:br>
</br>(See 
<xref rid="behggcij" type="fig"><html:a href="DSD0405014C8_02.xml#behggcij">Figure 1</html:a>
</xref>       .) 
</ttl>
<ol>
<li>
<p>Plug the AC cord directly into the AC outlet. Do not use an isolation transformer for this check.
</p>
</li>
<li>
<p>Connect a 1.5k&#8486;, 10 watts resistor, in parallel with a 0.15&#181;F capacitors, between each exposed metallic part on the set and a good earth ground such as a water pipe, as shown in 
<xref rid="behggcij" type="fig"><html:a href="DSD0405014C8_02.xml#behggcij">Figure 1</html:a>
</xref>.
</p>
</li>
<li>
<p>Use an AC voltmeter, with 1000 ohms&#47;volt or more sensitivity, to measure the potential across the resistor.
</p>
</li>
<li>
<p>Check each exposed metallic part, and measure the voltage at each point.
</p>
</li>
<li>
<p>Reverse the AC plug in the AC outlet and repeat each of the above measurements.
</p>
</li>
<li>
<p>The potential at any point should not exceed 0.75 volts RMS. A leakage current tester (Simpson Model 229 or equivalent) may be used to make the hot checks, leakage current must not exceed 1&#47;2 milliampere. In case a measurement isoutside
of the limits specified, there is a possibility of a shock hazard, and the equipment should be repaired and rechecked before it is returned to the customer.</p>
</li>
</ol>
</ti3>
</ti2>
</other>
</html:body>
</svctechdoc>
