Oriel 870
SC1058-M7816-HD Ver 1,0- RN1304
L5  3,3V F 1,35MHz
U13 1,8v 
L2 1,2V F 2,75MHz
U17 3,3V

LOG прошивки


SPI ID 0102154D (0102154D000000FF:9F)
Производитель Spansion
Название модели S25FL032P
Напряжение 3.30V
CMD частоты 33/66/66/66 МГц (Slow/Fast/Dual/Quad)
Размер страницы 0x100 (256)
Статус #1 0x9C (156)
Статус #2 0x00 (0)
Размер сектора 0x1000 (4 KiB)
Размер микросхемы 0x400000 (4 MiB)
SPI Дамп, 256 байт 
00000000 02 0B 00 00 00 BF 08 3C  0A 00 09 24 30 20 09 AD | .....?.<...$0 .­
00000010 00 BF 08 3C 00 00 09 24  40 57 09 AD 80 00 1A 3C | .?.<...$@W.­...<
00000020 00 68 9A 40 00 BF 08 3C  00 00 09 24 10 60 09 AD | .h.@.?.<...$.`.­
00000030 00 BF 08 3C 00 00 09 24  14 60 09 AD 0E 00 11 04 | .?.<...$.`.­....
00000040 00 00 00 00 20 BF 08 3C  01 00 09 24 00 67 09 AD | .... ?.<...$.g.­
00000050 20 BF 08 3C 02 00 09 24  00 67 09 AD 20 BF 08 3C |  ?.<...$.g.­ ?.<
00000060 03 00 09 24 00 67 09 AD  C0 BF 1F 3C 20 13 FF 27 | ...$.g.­A?.< .y'
00000070 08 00 E0 03 00 00 00 00  07 00 1A 24 00 90 9A 40 | ..a........$...@
00000080 00 00 00 00 00 00 00 00  00 98 80 40 00 00 00 00 | ...........@....
00000090 00 00 00 00 00 60 1A 40  00 DB 1A 00 09 00 60 07 | .....`.@.U....`.
000000A0 01 00 7B 33 E6 FF 1B 24  24 D0 5B 03 00 60 9A 40 | ..{3?y.$$?[..`.@
000000B0 00 60 1A 40 00 D3 1A 00  02 00 40 07 80 00 1A 3C | .`.@.O....@....<
000000C0 00 68 9A 40 00 00 00 00  00 48 80 40 00 58 80 40 | .h.@.....H.@.X.@
000000D0 00 80 08 40 00 80 09 3C  FF FF 29 35 24 40 09 01 | ...@...<yy)5$@..
000000E0 04 36 09 3C 25 40 09 01  00 80 88 40 00 60 08 40 | .6.<%@.....@.`.@
000000F0 FC FF 09 3C FF FF 29 35  24 40 09 01 00 00 09 24 | uy.<yy)5$@.....$
Сохранение данных в Файл C:/0/Oriel 870/Oriel 870.bin...Норма
Чтение SPI с адреса 0x00000000, размер 0x00400000...Норма
Завершено за 1.89 секунд(у). Скорость загрузки кода 2.12 MiB/сек.
Источник данных Файл C:/0/Oriel 870/Oriel 870.bin...Норма
Верификация SPI с адреса 0x00000000, размер 0x00400000...Норма
Завершено за 1.53 секунд(у). Скорость загрузки кода 2.61 MiB/сек.

++++++++++++++++++++++++++++
Analizator загрузки S25FL032P
SS 1pin
Miso 2pin
SCLK 6pin
Mosi 5pin
_________________________________
UART
MStar MSD7816 — 95, 94 TX Rx НА обратной стороне платы

[00]UART_115200

BIST0-OK

_snPD


PmRtcParam.u32RtcGetCounter=0x0000



PmRtcParam.u32RtcGetMatchCounter=0x0000


Hello U-Boot


U-Boot 1.1.6 (Aug 10 2012 - 02:08:15)

Board: MSTAR KRNOUS (CPU Speed 552 MHz)
DRAM:  64 X 0 MBytes
U-Boot is running at DRAM 0x87600000
Module: USB FAT FLASH SPI LOGO OSD ENV=SERIAL 
Flash is detected (0x0804, 0x01, 0x02, 0x15)
MDrv_SERFLASH_GetInfo()
	u32AccessWidth = 1
	u32TotalSize   = 4194304
	u32SecNum      = 64
	u32SecSize     = 65536
In:    serial
Out:   serial
Err:   serial
MSVC00B000100100208768TH0000000T
[do_set_paneltype][555] is invoked!! 
MDrv_PNL_Init u32PnlRiuBaseAddr = BF200000
MDrv_PNL_Init u32PMRiuBaseAddr = BF000000
MDrv_HDMITx_Init
Get IOMAP ID:300 Base:BF000000!
MDrv_HDMITx_SetHDMITxMode: HDMI mode 
DAC eTiming =6
HDMITx eTiming =7
MDrv_HDMITx_Exhibit: Create Check Rx timer success!
HDMITx eTiming =7
=>cmd: spi_rdc 0x80B2C000 0x20000 0x80
offset 0x20000, size 0x80
WARNING: it is better to set dram start addr aligned to 65536 !!!
WARNING: it is better to set total length aligned to 65536 !!!
Flash is detected (0x0804, 0x01, 0x02, 0x15)
initialization done!
logo addr in spi: 0xBFC70000; logo size:0xBA78
=>cmd: spi_rdc 0x80B2C000 0x70000 0xBA78
offset 0x70000, size 0xBA78
WARNING: it is better to set dram start addr aligned to 65536 !!!
WARNING: it is better to set total length aligned to 65536 !!!
u32ReadBuffVirAddr = A0000000, u32IntBuffVirAddr = A0100000, u32OutBuffVirAddr = A0730000
verJPD_SetStatus >>>>>>>>>>> w:720,  h:576,  p:720
GFX init--
GE_SetOnePixelMode
Hit any key to stop autoboot:  0 
WDT Initialize ... 
Start 75F2000 End 76A8000 
UnProtect MIU block 0 : 0x75F2000 0x76A8000
offset 0x8001C, size 0x28860D
WARNING: it is better to set flash start addr aligned to 65536 !!!
WARNING: it is better to set total length aligned to 65536 !!!
in=0x80B00000, in_size=0x28860D, out= 0x80000180, alloc_buf = 0x81000000 
in=0x80B00000, in_size=0x28860D, out= 0x80000180, alloc_buf = 0x81000000 
in_size=2655757 out_size=7535816 unpack_size=0 


LZMA Decompression...CRC_result 2144DF1C CRC_value 2144DF1C
CRC check success !!
ok

## Starting application at 0x80000224 ...
[cyg_net_init] Init: mbinit(0x00000000)
[cyg_net_init] Init: cyg_net_init_devs(0x00000000)
Init device 'pcnet_eth0'
[cyg_net_init] Init: loopattach(0x00000000)
[cyg_net_init] Init: ifinit(0x00000000)
[cyg_net_init] Init: domaininit(0x00000000)
[cyg_net_init] Init: cyg_net_add_domain(0x806d8548)
New domain internet at 0x00000000
[cyg_net_init] Init: cyg_net_add_domain(0x806d8110)
New domain route at 0x00000000
[cyg_net_init] Init: call_route_init(0x00000000)
[cyg_net_init] Done
[eCos][CPU INFO] : CPU Clock = 552000000 : RTC Period = 276000

Auth OK

Hardware Initialize...
MDrv_MIOMap_Init
[HAL_MIU_SetPMIOMapBase][1266] Non implement for MIU _gPM_MapBase= bf000000
MsOS_Init
_MApi_SystemInit_CreateMemoryPool
upoolSize = 320000 and u32Addr = 967438 
mdrv_gpio_init
MIU Initialize...
Get IOMap u32NonPmBase = 0xbf200000 
Get IOMap u32PmBase = 0xbf000000 
Disable MIU1 

 -----k1 U04----- 
WDT_Init 
MDrv_WDT_IsReset = 0
Hello Hummingbird!! 
_appDemo_Task.iId = 1985216513 
[_SysInit_InitAPI][1975]SPI Flash Driver Init !!
Flash is detected (0x0804, 0x01, 0x02, 0x15)
[HAL_AUDIO_AllocateVars], init Shared 


HAL_MAD_SetMemInfo[DSP_DEC] = 0x03b00000


HAL_MAD2_SetMemInfo[DSP_SE] = 0x03a00000


[HAL_AUDSP_DspLoadCode], pau_info->cm_len == 0
 ADEC Done and do default setting 4
===== Check Audio Decoder Protection from hash-key IP =====
Hash Key Check DD Fail, No DD license!!
Hash Key Check DDP Fail, No DD+ license!!
This is Demo Mode!!
Hash-key Support Generic HE-AAC !!
===== Check Protection IP End                         =====
MDrv_SERFLASH_GetInfo()
	u32AccessWidth = 1
	u32TotalSize   = 4194304
	u32SecNum      = 64
	u32SecSize     = 65536
MDrv_PNL_Init u32PnlRiuBaseAddr = bf200000
MDrv_PNL_Init u32PMRiuBaseAddr = bf000000
[XC,Version][1B][0;36m 00625983
 [1B][mDAC eTiming =6
DAC eTiming =6
HDMITx eTiming =7
Wait V Sync!!
GE_SetOnePixelMode
driver GE init ok
[_SysInit_GEGOP][1431]
[_SysInit_GEGOP][1439]

[GOP0, PID 0][Driver Version]: 0088, BuildNum: 0004, ChangeList: 2147483647
[_SysInit_GEGOP][1465]driver GOP0 init ok

[GOP1, PID 0][Driver Version]: 0088, BuildNum: 0004, ChangeList: 2147483647
[_SysInit_GEGOP][1465]driver GOP1 init ok

[GOP2, PID 0][Driver Version]: 0088, BuildNum: 0004, ChangeList: 2147483647
[_SysInit_GEGOP][1465]driver GOP2 init ok
Path2
Set to Mixer 

GOP_FUN_NOT_SUPPORTEDGE_Init and VE setting done
BASEADDRESS_STRING_DATABASE_IN_FLASH = 00370000 
BASEADDRESS_BITMAP_DATABASE_IN_FLASH = 00370000 
BASEADDRESS_GENSETTING_IN_FLASH = 00370000 
BASEADDRESS_CURRENT_DTV_ORDER_IN_FLASH = 00380000 
BASEADDRESS_CH_DATABASE_IN_FLASH = 00390000 
BASEADDRESS_MOSAIC_IN_FLASH = 003D0000 
BASEADDRESS_TFCA_MAIL_IN_FLASH = 003E0000 
NUMBER_OF_CURRENT_DTV_PROGRAM = 00001000 
USB init 
MDrv_Usb_Init..
Usb init
The base address is 0xA1739000
Base addr is 0xA1739000
Top addr is 0xA1758FFF
Pages per pool is 32
Bit map base addr is 0xa17387d0
usb_init start, UTMI base 0xbf205400, USBC base 0xbf220400, UHC base 0xbf220600
usb_hcd_cpe_ehci_probe
ehci: 80c86290
hcd: 80c862c4
The allocated addr is 0xa1739000, bit_map[0] is 0xFFFFFFFE
qh: 0xa1739000, qh->qh_dma: 0x01739000
The allocated addr is 0xa173a000, bit_map[0] is 0xFFFFFFFC
The allocated addr is 0xa173b000, bit_map[0] is 0xFFFFFFF8
qh: 0x01739000
usb_set_address  1 after
USB device product string (index 2) = CPE_AMBA EHCI
The allocated addr is 0xa173c000, bit_map[0] is 0xFFFFFFF0
<register_root_hub> hcd->rh_registered = 1
InitUSBIntr enter
Usb start..
MDrv_Usb_Done ...............................UsbTask..
..................
>>> Allocate Addr = A17356C0 , FwPhyAddr = 01735700 
************************ Start TSP_Init ************************
 <FWTSP> : >> FwVersion:002F2400 , Date:20120911 
************************* End TSP_Init *************************
[MApi_SI_System_Startup] OK !! 
MApi_DigiTuner_Init mutex id 1985216539 
MDrv_IIC_Init  PORT  1 
@@@@@@ u32CpuSpeedMHz= 552 MHz
#########[xinmer][MDrv_Demod_Init][4254] init star time 1257  
MDrv_DMD_MSB123xc_Init Init DVBC DSP Table By Device Driver ... 
MDrv_DMD_MSB123xc_Init Init DVBT DSP Table By Device Driver ... 
MDrv_DMD_MSB123xc_Init Init DVBT2 DSP Table By Device Driver ... 
_msbMSB123xc_set_bonding_option u16ChipID 2f
dvbt dsp reg init ok

[msb1236c]ver0 = 0x709, ver1 = 0x1
#########[xinmer][MDrv_Demod_Init][4309] init end time 4838
Nmi_Tuner_Interface_init_chip
before nmi_tuner_os_create_task
chipid: 120b0
nm131_chip_init id(120b0)
chipid: 120b0
chip id:[NMI] driver version (2.1.4.1) build 409
chipid: 120b0
[NMI] Chip ID:   1:20b0
nmi_tuner_os_create_task 222222222222222~~~~~~~~~~~
MApi_VectorFont_Init total size=3276800, free size=2819872, large size=2819828
alloc mem 0x330c
alloc mem 0x1f14
SysInit done .................................................
Nmi_Tuner_Task
into _appMain_Task 
[MApp_CheckFlash][1169] s8SN0 = 1 
MApi_DB_CM_LoadDTVProgramDatabaseFromFlash   -- u16Index[2322] [4096]
MApi_DB_CM_InitDTVDataManager: m_eCurrentServiceType = 1
MApi_DB_CM_InitDTVDataManager: m_wCurrentOrderOfTV = 4
MApi_DB_CM_InitDTVDataManager: m_wCurrentOrderOfRadio = 20
MApi_DB_CM_InitDTVDataManager: m_wCurrentOrderOfMosaic = 0
MApi_DB_CM_InitDTVDataManager: m_wCurrentOrderOfNvod_Ref = 0
MApi_DB_CM_InitDTVDataManager: m_wCurrentOrderOfNvod_TimeShifted = 0

#######[xinmer ]BK_BookEventInit   998    0

[MDrv_Demod_Restart]tuner demod Freq=602000, Bw=2,type=1,plpid=0
T2 dsp reg init ok
120 set tuner dwFreq(602000),ucBw(8)
tune: rf=602000000, if=4800000, bw=8, tvstd=14
Nmi_Tuner_Interface_Tuning
Nmi_Tuner_Interface_SelfTune:
tune.aif:0
tune.dacSel:2
tune.is_stereo:0
tune.output:2
tune.rf:602000000
tune.vif:4800000
tune.rfinvert:0
param->ucBw:8
param->tvstd:14
xo_f0     5dc0
 n0_fc8
 r8 64

 NMI_DRV_TUNE vif 4800000 , rf 602000000,std 12
gChipNowInfo.currentparam.freq(602000000) 
Nmi_Tuner_Interface_SelfTune end
Nmi_Tuner_Interface_Tuning end

[MSB1236C_DTV_SetFrequency]->freq=602000,bdwh=8,PlpID 0,type T2

setfreq T2
Set TSP0 registers...

reset T2
Tuner Success 
into appMain_AddApp 
[ZUI] init: sz_msg_q=6216
fix appTV_GetInfo before using 
YPBPR ON, CVBS ON, RGB OFF, HDMI ON
[msCHIP_DAC_SetOutputSource][156] input bitmap: 0x00000005
CVBS on
SVIDEO off, YPBPR on, RGB off
problem happen 
App_GetTVFormat:[0]
tvvideo_SetDCOutputTiming : 0, 1
Check the Source type 6 
[tvvideo_SetDCOutputTiming][502]: ## Change Resolution ##, eCompType = 6 
[msAPI_XC_ReMapComponentType][276]: msAPI_XC eTiming = 6
[_MDrv_PNL_Init_LPLL][286]pstPanelInitData->u16Width=1920, pstPanelInitData->u16Height=1080
[_MDrv_PNL_Init_LPLL][288]u16HTotal=2640,u16VTotal=1125,pstPanelInitData->u16HTotal=2640,pstPanelInitData->u16VTotal=1125, u16DefaultVFreq=500
[_MDrv_PNL_Init_Output_Dclk][345]pstPanelInitData->u16Width=1920, pstPanelInitData->u16Height=1080
[_MDrv_PNL_Init_Output_Dclk][347]u16HTotal=2640,u16VTotal=1125,pstPanelInitData->u16HTotal=2640,pstPanelInitData->u16VTotal=1125, u16DefaultVFreq=500
[_MDrv_PNL_Init_LPLL][286]pstPanelInitData->u16Width=1920, pstPanelInitData->u16Height=1080
[_MDrv_PNL_Init_LPLL][288]u16HTotal=2640,u16VTotal=1125,pstPanelInitData->u16HTotal=2640,pstPanelInitData->u16VTotal=1125, u16DefaultVFreq=500
[_MDrv_PNL_Init_Output_Dclk][345]pstPanelInitData->u16Width=1920, pstPanelInitData->u16Height=1080
[_MDrv_PNL_Init_Output_Dclk][347]u16HTotal=2640,u16VTotal=1125,pstPanelInitData->u16HTotal=2640,pstPanelInitData->u16VTotal=1125, u16DefaultVFreq=500
DAC eTiming =6
DAC eTiming =6
HDMITx eTiming =7
into appMain_AddApp 
into appMain_AddApp 
into appMain_AddApp 
[+]MApi_EpgDB_Init
[EPGDB][000711]  =========================================================================
[EPGDB][000712]  _pu16SrvMappingTable:  (Start, End, Length)= (0xa15a73e0, 0xa15a7430, 0x00000050)
[EPGDB][000713]  _pu8EitBufMask:        (Start, End, Length)= (0xa15a73c0, 0xa15a73c5, 0x00000005)
[EPGDB][000714]  _pMapBufIdxTable:      (Start, End, Length)= (0xa15a7220, 0xa15a73b0, 0x00000190)
[EPGDB][000715]  _pu8EpgDbEvtMask       (Start, End, Length)= (0xa15a6e20, 0xa15a7208, 0x000003e8)
[EPGDB][000716]  _pu8EpgDbScheHdrList   (Start, End, Length)= (0xa15a62d0, 0xa15a6e10, 0x00000b40)
[EPGDB][000717]  _pu8EpgDbSrvEvtList    (Start, End, Length)= (0xa159c540, 0xa15a62c0, 0x00009d80)
[EPGDB][000718]  _pu8EpgDbSrvSecList    (Start, End, Length)= (0xa1588530, 0xa159c530, 0x00014000)
[EPGDB][000719]  _pu8EpgDbEvtHdrList    (Start, End, Length)= (0xa1559720, 0xa1588520, 0x0002ee00)
[EPGDB][000720]  _pu8EpgDbEvtNameList   (Start, End, Length)= (0xa13637d0, 0xa1559710, 0x001f5f40)
[EPGDB][000721]  _pu8EpgDbPfHdrList     (Start, End, Length)= (0xa13636f0, 0xa13637b8, 0x000000c8)
[EPGDB][000722]  _pu8EpgDbPfPresent     (Start, End, Length)= (0xa13616e0, 0xa13636e0, 0x00002000)
[EPGDB][000723]  _pu8EpgDbPfFollow      (Start, End, Length)= (0xa135f6d0, 0xa13616d0, 0x00002000)
[EPGDB][000727]  _pu8EpgDbScheExtStrBuf      (Start, End, Length)= (0xa0e7f6c0, 0xa135f6c0, 0x004e0000)
[EPGDB][000729]  EPG database allocate 0x00727c95 bytes
[EPGDB][000735]  =========================================================================
[-]MApi_EpgDB_Init
MDrv_SERFLASH_GetInfo()
	u32AccessWidth = 1
	u32TotalSize   = 4194304
	u32SecNum      = 64
	u32SecSize     = 65536


App vserion $Change: 687715 $


[GOP3, PID 0][Driver Version]: 0088, BuildNum: 0004, ChangeList: 2147483647
MApp_ZUI_ACT_StartupOSD TV_PROG
[MApp_ZUI_ACT_PrepareOSDPage][437]MS_COMPONENT_OUTPUT_TYPE : 6 
fix _MApp_ZUI_SetupDisplayList before using
SD: 720 x 576, HD: 960 x 720
leave MApp_ZUI_API_InitCanvasGDI -> MApp_ZUI_API_GetFontMVF in 131
Set PAL
SD Gwin = 4
disp[1]'s FBID = 2
HD Gwin = 0 
[_ProcessFromWhere][1518][_ProcessFromWhere][1525]
[2394]  curPos_temp 4 PvrRecPosition  65535

[2395]  curPos_temp 0 PvrRecPosition  0

[2424]  _Estimate_Record_A_Play_B 0
_Zapper_Disable_AV: Enter at 8472.
alloc mem 0x2000
alloc mem 0x1000
alloc mem 0x40000
alloc mem 0x2400
Set PCR FLT=13 PID =      41B 

u32temp 0 
MIU0 u16MIUBankSelestion 0x0000
MIU0 Hi  0x003a
Video PID=0x41b,Flt=0xff
===== Check Audio Decoder Protection from hash-key IP =====
Hash Key Check DD Fail, No DD license!!
Hash Key Check DDP Fail, No DD+ license!!
This is Demo Mode!!
Hash-key Support Generic HE-AAC !!
===== Check Protection IP End                         =====
bSignalStatusChange 0
_Zapper_Disable_AV: Enter at 9449.
Set PCR FLT=13 PID =     1FFF 

