ÿ[00]UART_115200

BIST0-OK

_snPDMDrv_PM_RtcGetCounter(CurrentCounter=0)


Hello U-Boot


U-Boot 1.1.6 (Aug 26 2013 - 05:33:47)

Board: MSTAR KRNOUS (CPU Speed 552 MHz)
DRAM:  64 X 0 MBytes
U-Boot is running at DRAM 0x87600000
###############BOARD CONFIGURATION#####################
	DEFAULT ENBALE L2-Cache
	FPU(ENABLE)
	ENABLE_DDR3_16BIT_MODE
   DDR_FREQUENCY(1066MHz)
###############BOARD CONFIGURATION#####################
Module: USB FAT FLASH SPI LOGO OSD ENV=SERIAL 
Flash is detected (0x0804, 0x01, 0x02, 0x15)
MDrv_SERFLASH_GetInfo()
	u32AccessWidth = 1
	u32TotalSize   = 4194304
	u32SecNum      = 64
	u32SecSize     = 65536
In:    serial
Out:   serial
Err:   serial
MSVC00B000100100208768TH0000000T
[do_set_paneltype][764] is invoked!! 
MDrv_PNL_Init u32PnlRiuBaseAddr = BF200000
MDrv_PNL_Init u32PMRiuBaseAddr = BF000000
MDrv_HDMITx_Init
Get IOMAP ID:300 Base:BF000000!
MDrv_HDMITx_SetHDMITxMode: HDMI mode 
DAC eTiming =6
MDrv_HDMITx_SetHDMITxMode: HDMI mode 
HDMITx eTiming =7
MDrv_HDMITx_Exhibit: Create Check Rx timer success!
HDMITx eTiming =7
boot_logo=>cmd: spi_rdc 0x80B2C000 0x80000 0x11DA8
offset 0x80000, size 0x11DA8
WARNING: it is better to set dram start addr aligned to 65536 !!!
WARNING: it is better to set total length aligned to 65536 !!!
Flash is detected (0x0804, 0x01, 0x02, 0x15)
initialization done!
u32ReadBuffVirAddr = A0000000, u32IntBuffVirAddr = A0100000, u32OutBuffVirAddr = A0730000
verJPD_SetStatus >>>>>>>>>>> w:720,  h:576,  p:720
spi_rdc 0x80B00000 0x20000 0x1000
offset 0x20000, size 0x1000
WARNING: it is better to set total length aligned to 65536 !!!
cmd spi_rdc 0x80B00000 0x20000 0x1000 success
u32UbootInfoAddr: 0x91DA4
K1_INFO_ADDR: 0xA0000
spi_rdc 0x80B00000 0xA0000 0x1000
offset 0xA0000, size 0x1000
WARNING: it is better to set total length aligned to 65536 !!!
cmd spi_rdc 0x80B00000 0xA0000 0x1000 success
u32LogoMagicFlag ERROR !! return GOP_BUFFER_ADDR
GE_SetOnePixelMode
Hit any key to stop autoboot:  0 
WDT Initialize ... 
Start 75F2000 End 76A4000 
UnProtect MIU block 0 : 0x75F2000 0x76A4000
offset 0xA001C, size 0x291A5F
WARNING: it is better to set flash start addr aligned to 65536 !!!
WARNING: it is better to set total length aligned to 65536 !!!
in=0x80B00000, in_size=0x291A5F, out= 0x80000180, alloc_buf = 0x81000000 
in=0x80B00000, in_size=0x291A5F, out= 0x80000180, alloc_buf = 0x81000000 
in_size=2693727 out_size=7560180 unpack_size=0 


LZMA Decompression...CRC_result 1E376BDB CRC_value 1E376BDB
CRC check success !!
ok

## Starting application at 0x80000224 ...
[cyg_net_init] Init: mbinit(0x00000000)
[cyg_net_init] Init: cyg_net_init_devs(0x00000000)
Init device 'pcnet_eth0'
[cyg_net_init] Init: loopattach(0x00000000)
[cyg_net_init] Init: ifinit(0x00000000)
[cyg_net_init] Init: domaininit(0x00000000)
[cyg_net_init] Init: cyg_net_add_domain(0x806df198)
New domain internet at 0x00000000
[cyg_net_init] Init: cyg_net_add_domain(0x806ded60)
New domain route at 0x00000000
[cyg_net_init] Init: call_route_init(0x00000000)
[cyg_net_init] Done
[SysInit][1975]
[SysInit][1977]
****** Customer_info:Before ******
0xbx,0xbx,0xbx,0xbx,0xbx,0xbx,0xbx,0xbx,
0xbx,0xbx,0xbx,0xbx,0xbx,0xbx,0xbx,0xbx,
0xbx,0xbx,0xbx,0xbx,0xbx,0xbx,0xbx,0xbx,
0xbx,0xbx,0xbx,0xbx,0xbx,0xbx,0xbx,0xbx,
0xbx,0xbx,0xbx,0xbx,0xbx,0xbx,0xbx,0xbx,
0xbx,0xbx,0xbx,0xbx,0xbx,0xbx,0xbx,0xbx,
 abcdef => 0xbx,0xbx,0xbx,0xbx,0xbx,0xbx,
 ABCDEF => 0xbx,0xbx,0xbx,0xbx,0xbx,0xbx,

****** Customer_info ******
0xbx,0xbx,0xbx,0xbx,0xbx,0xbx,0xbx,0xbx,
0xbx,0xbx,0xbx,0xbx,0xbx,0xbx,0xbx,0xbx,
0xbx,0xbx,0xbx,0xbx,0xbx,0xbx,0xbx,0xbx,
0xbx,0xbx,0xbx,0xbx,0xbx,0xbx,0xbx,0xbx,
0xbx,0xbx,0xbx,0xbx,0xbx,0xbx,0xbx,0xbx,
0xbx,0xbx,0xbx,0xbx,0xbx,0xbx,0xbx,0xbx,[SysInit][1979]

Hash: ae0b4cdbb15b35b29f1b5f7a286b28f5
Auth OK

[SysInit][1981]
Hardware Initialize...
MDrv_MIOMap_Init
[HAL_MIU_SetPMIOMapBase][1107] Non implement for MIU _gPM_MapBase= bf000000
MsOS_Init
_MApi_SystemInit_CreateMemoryPool
upoolSize = 320000 and u32Addr = 96CCE0 
mdrv_gpio_init
[SysInit][1990]
MIU Initialize...
Get IOMap u32NonPmBase = 0xbf200000 
Get IOMap u32PmBase = 0xbf000000 
Disable MIU1 
[SysInit][1998]
WDT_Init 
[SysInit][2005]
[SysInit][2008]
MDrv_WDT_IsReset = 0
[SysInit][2014]
[MAPI_MEMINFO] DVBC System Memory Usage
[MAPI_MEMINFO] ============================ START         END           SIZE
[MAPI_MEMINFO] POOL_START                   0x00000000    0x016ce800    0x016ce800
[MAPI_MEMINFO] Cached Pool Start            0x0096cce0    0x00c8cce0    0x00320000
[MAPI_MEMINFO] NONCACHED_POOL_START         0x00c8cce0    0x016ce800    0x00a41b20
[MAPI_MEMINFO] 
[MAPI_MEMINFO] Memory Layout:
[MAPI_MEMINFO] ============================ START         END           SIZE
[MAPI_MEMINFO] XC_MEM_START                 0x03d00000    0x04000000    0x00300000
[MAPI_MEMINFO] MAD_MEM_START                0x03a00000    0x03d00000    0x00300000
[MAPI_MEMINFO] MVD_MEM_START                0x01d00000    0x03a00000    0x01d00000
[MAPI_MEMINFO] VE_MEM_START                 0x01b60000    0x01d00000    0x001a0000
[MAPI_MEMINFO] GOP_DMAMEM_START             0x01b5f000    0x01b60000    0x00001000
[MAPI_MEMINFO] TSP_VQ_START                 0x01b5e000    0x01b5f000    0x00001000
[MAPI_MEMINFO] PM51_MEM_ADR                 0x01b5dc00    0x01b5e000    0x00000400
[MAPI_MEMINFO] PM51_VAR_MEM_ADR             0x01b5d800    0x01b5dc00    0x00000400
[MAPI_MEMINFO] GOP_GWINMEM_START            0x016ce800    0x01b59800    0x0048b000

[MAPI_MEMINFO] pFirstAvailableMemory        0x8096cce0


[SysInit][2018]
[SysInit][2027]
Hello Hummingbird!! 
_appDemo_Task.iId = 1985216513 
----------Hello World----------
-------Welcome to Demo AP------
>> [_SysInit_InitAPI][1696]SPI Flash Driver Init !!
Flash is detected (0x0804, 0x01, 0x02, 0x15)
[HAL_AUDIO_AllocateVars], init Shared 


>> 

HAL_MAD_SetMemInfo[DSP_DEC] = 0x03b00000


HAL_MAD2_SetMemInfo[DSP_SE] = 0x03a00000

 ADEC Done and do default setting 4
===== Check Audio Decoder Protection from hash-key IP =====
Hash-key Support DD.
Hash-key Support DD+.
Hash-key Support Generic HE-AAC !!
Hash-key Support WMA.
===== Check Protection IP End                         =====
MDrv_SERFLASH_GetInfo()
	u32AccessWidth = 1
	u32TotalSize   = 4194304
	u32SecNum      = 64
	u32SecSize     = 65536
Check Boot Logo OK!! logo_cmd [boot_logo 0 0 1 1] 
Get Boot Panel Type!! 
pEnvStr = set_paneltype 12 
ptr = set_paneltype 12 
ptr+PANEL_CMD_LENGTH = 12 
result = 1 
result = 12 
g_PNL_TypeSel = 12 
eTiming =6
MDrv_PNL_Init u32PnlRiuBaseAddr = bf200000
MDrv_PNL_Init u32PMRiuBaseAddr = bf000000
[XC,Version][1B][0;36m 00516185
 [1B][mMApi_XC_Init, 438, pXC_InitData->stPanelInfo.eLPLL_Type=7
MDrv_HDMITx_Init
Get IOMAP ID:300 Base:bf000000!
MDrv_HDMITx_SetHDMITxMode: HDMI mode 
DAC eTiming =6
MDrv_HDMITx_SetHDMITxMode: HDMI mode 
HDMITx eTiming =7
MDrv_HDMITx_Exhibit: Create Check Rx timer success!
Wait V Sync!!
GE_SetOnePixelMode
driver GE init ok
[_SysInit_GEGOP][1266]
[_SysInit_GEGOP][1275]
[_SysInit_GEGOP][1301]driver GOP0 init ok
[_SysInit_GEGOP][1301]driver GOP1 init ok
[_SysInit_GEGOP][1301]driver GOP2 init ok
Path2
Set to Mixer 
GE_Init and VE setting done
BASEADDRESS_STRING_DATABASE_IN_FLASH = 00370000 
BASEADDRESS_BITMAP_DATABASE_IN_FLASH = 00370000 
BASEADDRESS_GENSETTING_IN_FLASH = 00370000 
BASEADDRESS_CURRENT_DTV_ORDER_IN_FLASH = 00380000 
BASEADDRESS_CH_DATABASE_IN_FLASH = 00390000 
BASEADDRESS_MOSAIC_IN_FLASH = 003D0000 
BASEADDRESS_TFCA_MAIL_IN_FLASH = 003E0000 
NUMBER_OF_CURRENT_DTV_PROGRAM = 00001000 
USB init 
MDrv_Usb_Init..
Usb init
The base address is 0xA169E000
Base addr is 0xA169E000
Top addr is 0xA16BDFFF
Pages per pool is 32
Bit map base addr is 0xa169d7d0
usb_init start, UTMI base bf205400, USBC base bf220400, UHC base bf220600
usb_hcd_cpe_ehci_probe
ehci: 80c89b20
hcd: 80c89b54
The allocated addr is 0xa169e000, bit_map[0] is 0xFFFFFFFE
qh: a169e000, qh->qh_dma: 169e000
The allocated addr is 0xa169f000, bit_map[0] is 0xFFFFFFFC
The allocated addr is 0xa16a0000, bit_map[0] is 0xFFFFFFF8
qh: 169e000
usb_new_device
usb_set_address before
usb_set_address after
The allocated addr is 0xa16a1000, bit_map[0] is 0xFFFFFFF0
InitUSBIntr enter
Usb start..
MDrv_Usb_Done ...........UsbTask..
......................................
>>> Allocate Addr = A169A6C0 , FwPhyAddr = 0169A700 
************************ Start TSP_Init ************************
 <FWTSP> : >> FwVersion:001B210E , Date:20100918 
************************* End TSP_Init *************************
[MApi_SI_System_Startup] OK !! 
[AP_NC_Alloc] Size = 1010 
[AP_C_Alloc] Size = 6be00 
[AP_NC_Alloc] Size = c8cf 
MApi_DigiTuner_Init mutex id 1985216536 
MDrv_IIC_Init  PORT  1 
@@@@@@ u32CpuSpeedMHz= 552 MHz
MDrv_DMD_MSB123xc_Init Init DVBC DSP Table By Device Driver ... 
MDrv_DMD_MSB123xc_Init Init DVBT DSP Table By Device Driver ... 
MDrv_DMD_MSB123xc_Init Init DVBT2 DSP Table By Device Driver ... 
_msbMSB123xc_set_bonding_option u16ChipID 2f
dvbt dsp reg init ok

[msb1236c]ver0 = 0x706, ver1 = 0x0
[Nmi Asic]: @ 8278: Chip ID (000120b0)
[Nmi Asic]: @ 8290: Chip ID (000120b0)
[NMI] NMI 120,13x driver version (2.1.2.5) build 323
[Nmi Asic]: @ 8298: Chip ID (000120b0)
[NMI] Chip ID = 0x000120b0
MApi_VectorFont_Init total size=3276800, free size=2815792, large size=2815748
alloc mem 0x330c
alloc mem 0x1f14
SysInit done .................................................
into _appMain_Task 
[MApp_CheckFlash][1200] s8SN0 = 1 
MApi_DB_CM_LoadDTVProgramDatabaseFromFlash   -- u16Index[3939] [4096]
MApi_DB_CM_InitDTVDataManager: m_eCurrentServiceType = 1
MApi_DB_CM_InitDTVDataManager: m_wCurrentOrderOfTV = 13
MApi_DB_CM_InitDTVDataManager: m_wCurrentOrderOfRadio = 20
MApi_DB_CM_InitDTVDataManager: m_wCurrentOrderOfMosaic = 0
MApi_DB_CM_InitDTVDataManager: m_wCurrentOrderOfNvod_Ref = 0
MApi_DB_CM_InitDTVDataManager: m_wCurrentOrderOfNvod_TimeShifted = 0
T2 dsp reg init ok

 #####tuner mode:0,506000,2,0,1###########################start demod restart scantype is 1

[MDrv_Demod_Restart]tuner demod Freq=506000, Bw=2,type=1,plpid=0
[Nmi Asic]: *** Notch Disable ***

[NMI]Change Frequency successful: freq = (506000000) Hz, IF = (4800000 Hz) BW = (8 MHz ).

[MSB1236C_DTV_SetFrequency]->freq=506000,bdwh=8,PlpID 0,type T2

setfreq T2
Set TSP0 registers...

reset T2
#################3demod restart success
Tuner Success 
into appMain_AddApp 
[ZUI] init: sz_msg_q=6216
fix appTV_GetInfo before using 
SCART ON, CVBS ON, RGB ON
[msCHIP_DAC_SetOutputSource][79] input bitmap: 0x00000011
CVBS on
SVIDEO off, YPBPR off, RGB on
SCART on
problem happen 
App_GetTVFormat:[4]
tvvideo_SetDCOutputTiming : 4, 1
Check the Source type e 

MDrv_HDMITx_SetAVMUTE 
[tvvideo_SetDCOutputTiming][564]: ## Change Resolution ##, eCompType = 14 
333##stSysSetting.u8TVFormat ===4####enResolutionType===14
[msAPI_XC_ReMapComponentType][293]: msAPI_XC eTiming = 2
DAC eTiming =2
MDrv_HDMITx_SetHDMITxMode: HDMI mode 
HDMITx eTiming =2
tvvideo_SetDCOutputTiming : 4, 1
Check the Source type e 

MDrv_HDMITx_SetAVMUTE 
[tvvideo_SetDCOutputTiming][564]: ## Change Resolution ##, eCompType = 14 
333##stSysSetting.u8TVFormat ===4####enResolutionType===14
[msAPI_XC_ReMapComponentType][293]: msAPI_XC eTiming = 2
DAC eTiming =2
MDrv_HDMITx_SetHDMITxMode: HDMI mode 
HDMITx eTiming =2
into appMain_AddApp 
into appMain_AddApp 
into appMain_AddApp 
[+]MApi_EpgDB_Init
[AP_NC_Alloc] Size = 50 
[AP_NC_Alloc] Size = 5 
[AP_NC_Alloc] Size = 190 
[AP_NC_Alloc] Size = 3e8 
[AP_NC_Alloc] Size = b40 
[AP_NC_Alloc] Size = 9d80 
[AP_NC_Alloc] Size = 14000 
[AP_NC_Alloc] Size = 2ee00 
[AP_NC_Alloc] Size = 1f5f40 
[AP_NC_Alloc] Size = c8 
[AP_NC_Alloc] Size = 2000 
[AP_NC_Alloc] Size = 2000 
[AP_NC_Alloc] Size = 4e0000 
[EPGDB][000711]  =========================================================================
[EPGDB][000712]  _pu16SrvMappingTable:  (Start, End, Length)= (0xa14cda20, 0xa14cda70, 0x00000050)
[EPGDB][000713]  _pu8EitBufMask:        (Start, End, Length)= (0xa14cda00, 0xa14cda05, 0x00000005)
[EPGDB][000714]  _pMapBufIdxTable:      (Start, End, Length)= (0xa14cd860, 0xa14cd9f0, 0x00000190)
[EPGDB][000715]  _pu8EpgDbEvtMask       (Start, End, Length)= (0xa14cd460, 0xa14cd848, 0x000003e8)
[EPGDB][000716]  _pu8EpgDbScheHdrList   (Start, End, Length)= (0xa14cc910, 0xa14cd450, 0x00000b40)
[EPGDB][000717]  _pu8EpgDbSrvEvtList    (Start, End, Length)= (0xa14c2b80, 0xa14cc900, 0x00009d80)
[EPGDB][000718]  _pu8EpgDbSrvSecList    (Start, End, Length)= (0xa14aeb70, 0xa14c2b70, 0x00014000)
[EPGDB][000719]  _pu8EpgDbEvtHdrList    (Start, End, Length)= (0xa147fd60, 0xa14aeb60, 0x0002ee00)
[EPGDB][000720]  _pu8EpgDbEvtNameList   (Start, End, Length)= (0xa1289e10, 0xa147fd50, 0x001f5f40)
[EPGDB][000721]  _pu8EpgDbPfHdrList     (Start, End, Length)= (0xa1289d30, 0xa1289df8, 0x000000c8)
[EPGDB][000722]  _pu8EpgDbPfPresent     (Start, End, Length)= (0xa1287d20, 0xa1289d20, 0x00002000)
[EPGDB][000723]  _pu8EpgDbPfFollow      (Start, End, Length)= (0xa1285d10, 0xa1287d10, 0x00002000)
[EPGDB][000727]  _pu8EpgDbScheExtStrBuf      (Start, End, Length)= (0xa0da5d00, 0xa1285d00, 0x004e0000)
[EPGDB][000729]  EPG database allocate 0x00727c95 bytes
[EPGDB][000735]  =========================================================================
[-]MApi_EpgDB_Init
MDrv_SERFLASH_GetInfo()
	u32AccessWidth = 1
	u32TotalSize   = 4194304
	u32SecNum      = 64
	u32SecSize     = 65536
MApp_ZUI_ACT_StartupOSD TV_PROG
[MApp_ZUI_ACT_PrepareOSDPage][436]MS_COMPONENT_OUTPUT_TYPE : 14 
fix _MApp_ZUI_SetupDisplayList before using
SD: 720 x 576, HD: 720 x 576
leave MApp_ZUI_API_InitCanvasGDI -> MApp_ZUI_API_GetFontMVF in 131
Set PAL
SD Gwin = 4
disp[1]'s FBID = 2
HD Gwin = 0 
[_ProcessFromWhere][1578][_ProcessFromWhere][1585]
[2522]  curPos_temp 13 PvrRecPosition  65535

[2523]  curPos_temp 0 PvrRecPosition  0

[2552]  _Estimate_Record_A_Play_B 0
_Zapper_Disable_AV: Enter at 11388.

[_Zapper_TaskState_TUNER]get current demod type 1,plpid 0

 #####tuner mode:0,506000,2,0,1Set PCR FLT=13 PID =      7F9 

Video PID=0x7f9,Flt=0xff
===== Check Audio Decoder Protection from hash-key IP =====
Hash-key Support DD.
Hash-key Support DD+.
Hash-key Support Generic HE-AAC !!
Hash-key Support WMA.
===== Check Protection IP End                         =====
bSignalStatusChange 1
bSignalStatusChange 0
_Zapper_Disable_AV: Enter at 17521.
alloc mem 0x40000
alloc mem 0x2400
alloc mem 0x2000
alloc mem 0x1000
Set PCR FLT=13 PID =     1FFF 

bSignalStatusChange 1
Buffer id ?? 
bSignalStatusChange 0
_Zapper_Disable_AV: Enter at 20186.
bSignalStatusChange 1
Buffer id ?? 
bSignalStatusChange 0
_Zapper_Disable_AV: Enter at 22861.
bSignalStatusChange 1
Buffer id ?? 
bSignalStatusChange 0
_Zapper_Disable_AV: Enter at 25536.
