<?xml version="1.0" encoding="utf-8"?>
<?xml-stylesheet href="DSD0405014C8.css" type="text/css"?>
<!-- DC Version =\\\\\\\\ "(unknown).0.0.1" -->
<!-- Character entity set. Typical invocation:
     <!ENTITY % ISOnum PUBLIC
       "ISO 8879-1986//ENTITIES Numeric and Special Graphic//EN">
     %ISOnum;
-->
<svctechdoc lang="english" type="svc" xmlns:html="http://www.w3.org/Profiles/XHTML-transitional">
<html:script language="JavaScript" src="script.js"></html:script>
<html:script language="JavaScript" src="tree.js"></html:script>
<html:body onload="dgfFsetClose();setScroll();">
<other>
<ttl><html:a name="TITLE7">7 Taking out the Disc from RAM-Drive Unit when the Disc cannot be ejected by OPEN &#47; CLOSE button </html:a>
</ttl>
<ti2 column="3">
<ttl><html:a name="TITLE7_1">7.1 Forcible Disc Eject </html:a>
</ttl>
<ti3 module="0">
<ttl><html:a name="TITLE7_1_1">7.1.1 When the power can be turned off. </html:a>
</ttl>
<ol>
<li>
<p>Turn off the power and press [STOP] [CH UP] keys on the front panel simultaneously for 5 seconds.
</p>
</li>
</ol>
</ti3>
<ti3 module="0">
<ttl><html:a name="TITLE7_1_2">7.1.2 When the power can not be turned off. </html:a>
</ttl>
<ol>
<li>
<p>Press [POWER] key on the front panel for over 10 seconds to turn off the power forcibly, and press [STOP] [CH UP] keys on the front panel simultaneously for 5 seconds.
</p>
</li>
</ol>
</ti3>
</ti2>
<ti2 column="3">
<ttl><html:a name="TITLE7_2">7.2 When the Forcible Disc Eject can not be done. </html:a>
</ttl>
<ol>
<li>
<p>Turn off the power and pull out AC cord.
</p>
</li>
<li>
<p>Remove the Top Case.
</p>
</li>
<li>
<p>Remove the Front Panel.
</p>
</li>
<li>
<p>Remove 4 screws and Upper Base Unit from DVD-RAM Drive.
</p>
</li>
<li>
<p>Take out the disc and put the Opener Roller on fully position for direction of Arrow.
</p>
</li>
<li>
<p>Put the Upper Base Unit so that the Opener Roller is inserted into the groove.
</p>
</li>
<li>
<p>Check center of Opener Roller is seen through the Opener position Checking Hole, and tighten 4 screws.
</p>
</li>
</ol>
<fig>
<graphic loc="graphic8" sizex="157.311mm" sizey="154.517mm"><html:img src="re_fde01.png" border="0"></html:img>
</graphic>
</fig>
</ti2>
</other>
</html:body>
</svctechdoc>
